{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / AZQS-BY1 A"]
[]
[]
[]
[]
["","","","","FCQG100FVEB / AZQS100B7Y1B A","FCQG125FVEB / AZQS125B7Y1B A","FCQG140FVEB / AZQS140B7Y1B A"]
["Cooling capacity","Nom.","","kW","9.5","12.1","13.0"]
["Heating capacity","Nom.","","kW","10.8","13.5","15.5"]
["الفعالية الاسمية","نسبة فعالية استهلاك الطاقة","","","3.21","3.10","2.81"]
["","عامل الأداء","","","3.50","3.41","3.30"]
["","استهلاك الطاقة السنوي","","kWh","1,480","1,952","2,313"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","B"]
["","","تدفئة","","B","B"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A"]
["","الاستطاعة","Pdesign","kW","9.50"]
["","SEER","","","5.50"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","605"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A"]
["","الاستطاعة","Pdesign","kW","7.60"]
["","SCOP/A","","","3.85"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","2,764"]
["Notes","","","","(1) - يتوافق الاستهلاك السنوي للطاقة مع توجيه الطاقة الملصق 2002/31/EC","(1) - يتوافق الاستهلاك السنوي للطاقة مع توجيه الطاقة الملصق 2002/31/EC","(1) - يتوافق الاستهلاك السنوي للطاقة مع توجيه الطاقة الملصق 2002/31/EC"]
["","","","","(2) - يتوافق SEER وSCOP مع EN 14825","(2) - يتوافق SEER وSCOP مع EN 14825","(2) - يتوافق SEER وSCOP مع EN 14825"]
["","","","","(3) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(3) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(3) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]