{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":14,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / FCQG35FVEB / RZQG71L8Y1B","FCQG100FVEB / RZQG71L8Y1B","FCQG71FVEB / RZQG71L8Y1B","FCQG140FVEB / RZQG100L8Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L8Y1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG100L8Y1B","FCQG71FVEB / FCQG71FVEB / RZQG100L8Y1B","FCQG140FVEB / RZQG125L8Y1B","FCQG71FVEB / FCQG71FVEB / RZQG125L8Y1B","FCQG140FVEB / RZQG140L7Y1B"]
["Cooling capacity","Nom.","","kW","","","6.8","","","","","","","13.4"]
["تبريد المساحة","SEER","","","5.1","6.80","6.72","6.80","5.10","5.10","5.10","6.00","5.10"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","467","350","355","489","652","652","652","700","824"]
["","الاستطاعة","Pdesign","kW","6.8","6.80","6.80","9.50","9.50","9.50","9.50","12.00","12.00"]
["","فئة فعالية استهلاك الطاقة","","","B","A++","A++","A++","B","B","B","A+","B"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","6","6.33","6.33","11.30","11.30","11.30","11.30","12.66","12.71"]
["","SCOP/A","","","3.8","4.20","4.20","4.61","3.80","3.80","3.80","4.10","3.80"]
["","فئة فعالية استهلاك الطاقة","","","A","A+","A+","A++","A","A","A","A+","A"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","2,211","2,110","2,110","3,432","4,164","4,164","4,164","4,323","4,683"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","","","1,005"]
["","نسبة فعالية استهلاك الطاقة","","","","","3.39","","","","","","","3.21"]
["","عامل الأداء","","","","","3.97","","","","","","","3.61"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","","A"]
["","","تدفئة","","","","A"]
["Heating capacity","Nom.","","kW","","","7.5","","","","","","","15.5"]
["Notes","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","","","(1) - يتوافق الاستهلاك السنوي للطاقة مع توجيه الطاقة الملصق 2002/31/EC","","","","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","","","(2) - يتوافق SEER وSCOP مع EN 14825","","","","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]