{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQH-D"]
[]
[]
[]
[]
["","","","","FCQH71D7VEB","FCQH100D7VEB","FCQH125D7VEB","FCQH140D7VEB"]
["Sound pressure level","Heating","High","dBA","36","45","45","45"]
["","","Low","dBA","28","32","36","38"]
["","Cooling","Low","dBA","28","32","36","38"]
["","","High","dBA","36","45","45","45"]
["Standard Accessories","دليل التركيب والتشغيل","","","دليل التركيب والتشغيل","دليل التركيب والتشغيل","دليل التركيب والتشغيل","دليل التركيب والتشغيل"]
["","خرطوم الصرف","","","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف"]
["","مشبك لخرطوم الصرف","","","مشبك لخرطوم الصرف","مشبك لخرطوم الصرف","مشبك لخرطوم الصرف","مشبك لخرطوم الصرف"]
["","حلقة للدعامة الحاملة","","","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة"]
["","مسامير لولبية","","","مسامير لولبية","مسامير لولبية","مسامير لولبية","مسامير لولبية"]
["","دليل التركيب","","","دليل التركيب","دليل التركيب","دليل التركيب","دليل التركيب"]
["","عازل لأدوات التثبيت","","","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت"]
["","لبادة مانعة للتسريب","","","لبادة مانعة للتسريب","لبادة مانعة للتسريب","لبادة مانعة للتسريب","لبادة مانعة للتسريب"]
["","لبادة مانعة التسريب للمصرف","","","لبادة مانعة التسريب للمصرف","لبادة مانعة التسريب للمصرف","لبادة مانعة التسريب للمصرف","لبادة مانعة التسريب للمصرف"]
["Piping connections","Liquid","القطر الخارجي","mm","9.52","9.52","9.52","9.52"]
["","غاز","القطر الخارجي","mm","15.9","15.9","15.9","15.9"]
["","Drain","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Sound power level","التبريد","","dBA","54","62","62","62"]
["Dimensions","Unit","العرض","mm","840","840","840","840"]
["","","العمق","mm","840","840","840","840"]
["","","الارتفاع","mm","246","288","288","288"]
["الغلاف","المادة","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["الوزن","الوحدة","","kg","23","25","25","25"]
["لوحة ديكور","الوزن","","kg","5.5","5.5","5.5","5.5"]
["","الطراز","","","BYCQ140CW1","BYCQ140CW1","BYCQ140CW1","BYCQ140CW1"]
["","الأبعاد","الارتفاع","mm","50","50","50","50"]
["","","العمق","mm","950","950","950","950"]
["","","العرض","mm","950","950","950","950"]
["","اللون","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["Power supply","الطور","","","1~","1~","1~","1~"]
["","Frequency","","Hz","50/60","50/60","50/60","50/60"]
["","الاسم","","","VE","VE","VE","VE"]
["","Voltage","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","(1) - The sound power level is an absolute value indicating the power which a sound source generates.","(1) - The sound power level is an absolute value indicating the power which a sound source generates.","(1) - The sound power level is an absolute value indicating the power which a sound source generates.","(1) - The sound power level is an absolute value indicating the power which a sound source generates."]
["","","","","(2) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(2) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(2) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt.","(2) - The BYCQ140CW1W has white insulations.  Be informed that formation of dirt on white insulations is more visible and that it is consequently not advised to install the BYCQ140W1W decoration panel in environments exposed to concentrations of dirt."]