{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["الغلاف","المادة","","","","Zinc coated low carbon steel","Zinc coated low carbon steel"]
["الأبعاد","الوحدة","","الارتفاع","mm","230","230"]
["","","","العرض","mm","652","652"]
["","","","العمق","mm","502","502"]
["الوزن","الوحدة","","","kg","17.0","17.0"]
["Fan","Air flow rate","Cooling","High","m³/min","6.50","6.50"]
["","","","Low","m³/min","5.20","5.20"]
["","","Heating","High","m³/min","6.95","6.95"]
["","","","Low","m³/min","5.20","5.20"]
["مستوى طاقة الصوت","التبريد","","","dBA","55","55"]
["","التدفئة","","","dBA","55","55"]
["Sound pressure level","Cooling","","High","dBA","35.0","35.0"]
["","","","Low","dBA","28.0","28.0"]
["","Heating","","High","dBA","35.0","35.0"]
["","","","Low","dBA","29.0","29.0"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.52","9.52"]
["","التصريف","","","","27.2","27.2"]
["أنظمة التحكم","جهاز تحكم عن بُعد سلكي","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Standard Accessories","دليل التركيب والتشغيل","","","","1","1"]
["","مرشح هواء الشفط","","","","1","1"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1"]
["","الطور","","","","1~","1~"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","V","230","230 +/-10%"]
["Notes","","","","","(1) - يتم قياس قيم الصوت في غرفة شبه كاتمة للصدى.","(1) - يتم قياس قيم الصوت في غرفة شبه كاتمة للصدى."]
["","","","","","(2) - مستوى ضغط الصوت هو قيمة نسبية، تعتمد على المسافة والبيئة الصوتية. لمزيد من التفاصيل، يرجى الرجوع إلى مخططات مستوى الصوت.","(2) - مستوى ضغط الصوت هو قيمة نسبية، تعتمد على المسافة والبيئة الصوتية. لمزيد من التفاصيل، يرجى الرجوع إلى مخططات مستوى الصوت."]
["","","","","","(3) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(3) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت."]