{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDEQ-B"]
[]
[]
[]
[]
["","","","","FDEQ71B8V3B","FDEQ100B8V3B","FDEQ125B8V3B"]
["Sound pressure level","Heating","High","dBA","37.0","39.0","41.0"]
["","","Low","dBA","33.0","34.0","35.0"]
["","Cooling","Low","dBA","33.0","34.0","35.0"]
["","","High","dBA","37.0","39.0","41.0"]
["Standard Accessories","دليل التركيب والتشغيل","","","1","1","1"]
["Piping connections","Liquid","القطر الخارجي","mm","9.52","9.52","9.52"]
["","غاز","القطر الخارجي","mm","15.9","15.9","15.9"]
["","Drain","","","32","32","32"]
["مطلوب مسافة فوق السقف المستعار >","mm","","","290","290","290"]
["Sound power level","التبريد","","dBA","63.0","65.0","66.0"]
["Dimensions","Unit","العرض","mm","987","987","1,387"]
["","","العمق","mm","750","750","750"]
["","","الارتفاع","mm","279","279","279"]
["الغلاف","المادة","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["","اللون","","","Unpainted","Unpainted","Unpainted"]
["الوزن","الوحدة","","kg","38.1","38.1","48.6"]
["Fan","External static pressure","عالٍ","باسكال","100","100","100"]
["","","الإسمي","باسكال","50","50","50"]
["","","منخفض","باسكال","25","25","25"]
["Power supply","الطور","","","1~","1~","1~"]
["","Frequency","","Hz","50","50","50"]
["","الاسم","","","V3","V3","V3"]
["","Voltage","","V","230","230","230"]
["Notes","","","","(1) - Sound values are measured in a semi-anechoic room.","(1) - Sound values are measured in a semi-anechoic room.","(1) - Sound values are measured in a semi-anechoic room."]
["","","","","(2) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(2) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(2) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings."]
["","","","","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates."]