{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":8,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDEQ-B"]
[]
[]
[]
[]
["","","","","","FDEQ71B8V3B","FDEQ100B8V3B","FDEQ125B8V3B"]
["مروحة","الضغط الاستاتيكي الخارجي","","عالٍ","باسكال","100","100","100"]
["","","","منخفض","باسكال","25","25","25"]
["الغلاف","اللون","","","","Unpainted","Unpainted","Unpainted"]
["","المادة","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["الأبعاد","الوحدة","","الارتفاع","mm","279","279","279"]
["","","","العرض","mm","987","987","1387"]
["","","","العمق","mm","750","750","750"]
["الوزن","الوحدة","","","kg","38.1","38.1","48.6"]
["مطلوب مسافة فوق السقف المستعار >-=-مم","mm","","","","290","290","290"]
["Fan","Air flow rate","Cooling","High","m³/min","19","27","35"]
["","","","Low","m³/min","14","20","24"]
["","","Heating","High","m³/min","19","27","35"]
["","","","Low","m³/min","14","20","24"]
["مروحة","الضغط الاستاتيكي الخارجي","","الإسمي","باسكال","50","50","50"]
["مستوى طاقة الصوت","التبريد","","","dBA","63","65","66"]
["Sound pressure level","Cooling","","High","dBA","37","39","41"]
["","","","Low","dBA","33","34","35"]
["","Heating","","High","dBA","37","39","41"]
["","","","Low","dBA","33","34","35"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","15.9","15.9","15.9"]
["","التصريف","","","","32","32","32"]
["Standard Accessories","دليل التركيب والتشغيل","","","","1","1","1"]
["وحدة التزويد بالطاقة","الاسم","","","","V3","V3","V3"]
["","الطور","","","","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","230","230","230"]
["Notes","","","","","(1) - يتم قياس قيم الصوت في غرفة شبه كاتمة للصدى.","(1) - يتم قياس قيم الصوت في غرفة شبه كاتمة للصدى.","(1) - يتم قياس قيم الصوت في غرفة شبه كاتمة للصدى."]
["","","","","","(2) - مستوى ضغط الصوت هو قيمة نسبية، تعتمد على المسافة والبيئة الصوتية. لمزيد من التفاصيل، يرجى الرجوع إلى مخططات مستوى الصوت.","(2) - مستوى ضغط الصوت هو قيمة نسبية، تعتمد على المسافة والبيئة الصوتية. لمزيد من التفاصيل، يرجى الرجوع إلى مخططات مستوى الصوت.","(2) - مستوى ضغط الصوت هو قيمة نسبية، تعتمد على المسافة والبيئة الصوتية. لمزيد من التفاصيل، يرجى الرجوع إلى مخططات مستوى الصوت."]
["","","","","","(3) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(3) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(3) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت."]