{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDKS-C"]
[]
[]
[]
[]
["","","","","FDKS50C7VMB","FDKS50CVMB","FDKS60CVMB","FDKS60C7VMB"]
["Sound pressure level","Cooling","Silent operation","dBA","31.0","31.0","32.0","32.0"]
["","","Low","dBA","33.0","33.0","34.0","34.0"]
["","","High","dBA","37.0","37.0","38.0","38.0"]
["","","Nom.","dBA","35.0","35.0","36.0","36.0"]
["Standard Accessories","دليل التركيب","","","1","1","1","1"]
["","دليل التشغيل","","","1","1","1","1"]
["","جهاز تحكم عن بعد بالأشعة تحت الحمراء","","","","1","1"]
["","البطاريات","","","2","2","2","2"]
["","حامل جهاز التحكم عن بعد","","","1","1","1","1"]
["","مسمار تثبيت لولبي لجهاز التحكم عن بعد","","","2","2","2","2"]
["","مجموعة غطاء مستقبل الإشارة","","","1","1","1","1"]
["","عازل لأدوات التثبيت","","","1","1","1","1"]
["","لبادة مانعة للتسريب","","","1","1","1","1"]
["","مشبك معدني","","","1","1","1","1"]
["","خرطوم الصرف","","","1","1","1","1"]
["","حلقة للدعامة الحاملة","","","8","8","8","8"]
["","مواد مانعة للتسريب","","","2","2","2","2"]
["","مشابك","","","6","6","6","6"]
["","حلقة للوحة التثبيت","","","4","4","4","4"]
["","مسامير لولبية لشفة مجاري الهواء","","","1","1","1","1"]
["","مرشح هواء","","","1","1","1","1"]
["Sound power level","التبريد","","dBA","55.0","55.0","56.0","56.0"]
["Dimensions","Unit","العرض","mm","900","900","1,100","1,100"]
["","","العمق","mm","620","620","620","620"]
["","","الارتفاع","mm","200","200","200","200"]
["الوزن","الوحدة","","kg","27.0","27.0","30.0","30.0"]
["Fan","External static pressure","الإسمي","باسكال","40","40","40","40"]
["Power supply","الطور","","","1~","1~","1~","1~"]
["","Frequency","","Hz","50/60","50/60","50/60","50/60"]
["","الاسم","","","VM","VM","VM","VM"]
["","Voltage","","V","220-240/220-230","220-240/220-230","220-240/220-230","220-240/220-230"]
["Notes","","","","","(1) - يتم قياس قيم الصوت في غرفة كاتمة للصدى.","(1) - يتم قياس قيم الصوت في غرفة كاتمة للصدى."]
["","","","","","(2) - مستوى ضغط الصوت هو قيمة نسبية، تعتمد على المسافة والبيئة الصوتية. لمزيد من التفاصيل، يرجى الرجوع إلى مخططات مستوى الصوت.","(2) - مستوى ضغط الصوت هو قيمة نسبية، تعتمد على المسافة والبيئة الصوتية. لمزيد من التفاصيل، يرجى الرجوع إلى مخططات مستوى الصوت."]
["","","","","","(3) - مستوى قوة الصوت هو القيمة المطلقة التي يولدها مصدر الصوت.","(3) - مستوى قوة الصوت هو القيمة المطلقة التي يولدها مصدر الصوت."]
["Standard Accessories","جهاز تحكم عن بعد لاسلكي","","","1","","","1"]
["Notes","","","","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء","","","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء"]