{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQ-BW1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RZQ125B8W1B"]
["Cooling capacity","Nom.","","kW","12.50 (1)"]
["Piping connections","Liquid","القطر الخارجي","mm","9.52"]
["","غاز","القطر الخارجي","mm","15.9"]
["","Drain","OD","mm","26"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","2,075"]
["","نسبة فعالية استهلاك الطاقة","","","3.01"]
["","عامل الأداء","","","3.79"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","B"]
["","","تدفئة","","A"]
["Heating capacity","Nom.","","kW","14.00 (2)"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","(3) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]