{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B"]
[]
[]
[]
[]
["","","","","","FDQ125B8V3B9","FDQ200B8V3B9","FDQ250B8V3B9"]
["Cooling capacity","Total capacity","","Nom.","kW","","20.0","24.1"]
["Heating capacity","الاستطاعة الإجمالية","","الإسمي","kW","","23.0","26.4"]
["الغلاف","اللون","","","","Unpainted","Unpainted","Unpainted"]
["","المادة","","","","Galvanised steel","Galvanised steel","Galvanised steel"]
["Dimensions","Unit","","الارتفاع","mm","350","450","450"]
["","","","العرض","mm","1,400","1,400","1,400"]
["","","","العمق","mm","662","900","900"]
["الوزن","الوحدة","","","kg","59.0","89.0","94.0"]
["مطلوب مسافة فوق السقف المستعار >","mm","","","","350","450","450"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","43.0"]
["","","","متوسط","m³/min","","69.0","89.0"]
["","","Heating","Nom.","m³/min","43.0"]
["","","","متوسط","m³/min","","69.0","89.0"]
["","External static pressure","","عالٍ","باسكال","150","250","250"]
["","","","الإسمي","باسكال","150","250","250"]
["","","","منخفض","باسكال","150","250","250"]
["Sound power level","التبريد","","","dBA","75.0","81.0","82.0"]
["Sound pressure level","Cooling","","High","dBA","44.0","45.0","47.0"]
["","Heating","","Low","dBA","44.0","45.0","47.0"]
["Piping connections","Liquid","","القطر الخارجي","mm","9.52","9.52","12.70"]
["","غاز","","القطر الخارجي","mm","15.9","22.2","22.2"]
["","Drain","","","","","OD Ø25.0","OD Ø25.0"]
["أنظمة التحكم","Wired remote control","","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Standard Accessories","دليل التركيب والتشغيل","","","","1","1","1"]
["Power supply","الاسم","","","","V3","V3","V3"]
["","الطور","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","230","230 +/-10%","230 +/-10%"]
["Notes","","","","","(1) - يتم قياس قيم مستوى الصوت في غرفة شبه كاتمة للصدى مع التصحيح.","(1) - يتم قياس قيم مستوى الصوت في غرفة شبه كاتمة للصدى مع التصحيح.","(1) - يتم قياس قيم مستوى الصوت في غرفة شبه كاتمة للصدى مع التصحيح."]
["","","","","","(2) - يتم قياس مستوى ضغط الصوت عبر ميكروفون على مسافة 1 متر من الوحدة.","(2) - يتم قياس مستوى ضغط الصوت عبر ميكروفون على مسافة 1 متر من الوحدة.","(2) - يتم قياس مستوى ضغط الصوت عبر ميكروفون على مسافة 1 متر من الوحدة."]
["","","","","","(3) - مستوى ضغط الصوت هو قيمة نسبية، تعتمد على المسافة والبيئة الصوتية. لمزيد من التفاصيل، يرجى الرجوع إلى مخططات مستوى الصوت.","(3) - مستوى ضغط الصوت هو قيمة نسبية، تعتمد على المسافة والبيئة الصوتية. لمزيد من التفاصيل، يرجى الرجوع إلى مخططات مستوى الصوت.","(3) - مستوى ضغط الصوت هو قيمة نسبية، تعتمد على المسافة والبيئة الصوتية. لمزيد من التفاصيل، يرجى الرجوع إلى مخططات مستوى الصوت."]
["","","","","","(4) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(4) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(4) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت."]
["","","","","","(5) - لمزيد من التفاصيل، يرجى الرجوع إلى مخطط الأسلاك ولوحة الاسم ودليل التركيب.","(5) - لمزيد من التفاصيل، يرجى الرجوع إلى مخطط الأسلاك ولوحة الاسم ودليل التركيب.","(5) - لمزيد من التفاصيل، يرجى الرجوع إلى مخطط الأسلاك ولوحة الاسم ودليل التركيب."]