{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDQ125C7VEB / RZQSG125L8Y1B","FDQ125C5VEB / RZQSG125L8Y1B"]
["Cooling capacity","Nom.","","kW","12.0","12.0"]
["تبريد المساحة","SEER","","","5.2","5.2"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","808","808"]
["","الاستطاعة","Pdesign","kW","12","12"]
["","فئة فعالية استهلاك الطاقة","","","A","A"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","7.6","7.6"]
["","SCOP/A","","","3.9","3.9"]
["","فئة فعالية استهلاك الطاقة","","","A","A"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","2,729","2,729"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","1,870","1,870"]
["","نسبة فعالية استهلاك الطاقة","","","3.21","3.21"]
["","عامل الأداء","","","3.51","3.51"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A"]
["","","تدفئة","","B","B"]
["Heating capacity","Nom.","","kW","13.5","13.5"]
["Notes","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]