{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / 3MXM-N"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B / FDXM25F3V1B / 3MXM52N2V1B"]
["Cooling capacity","Nom.","","kW","5.0"]
["تبريد المساحة","SEER","","","6.36"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","276"]
["","الاستطاعة","Pdesign","kW","5.00"]
["","فئة فعالية استهلاك الطاقة","","","A++"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","4.80"]
["","SCOP/A","","","3.83"]
["","فئة فعالية استهلاك الطاقة","","","A"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","1,754"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","606"]
["","نسبة فعالية استهلاك الطاقة","","","4.12"]
["","عامل الأداء","","","3.69"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A"]
["","","تدفئة","","A"]
["Heating capacity","Nom.","","kW","6.80"]
["Notes","","","","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]