{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RXM-N"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B / RXM50N2V1B","FDXM60F3V1B / RXM60N2V1B"]
["Cooling capacity","Min.","","kW","","1.70"]
["","Nom.","","kW","","6.00"]
["","Max.","","kW","","6.50"]
["Heating capacity","Min.","","kW","","1.70"]
["","Nom.","","kW","","7.00"]
["","Max.","","kW","","7.10"]
["الفعالية الاسمية","نسبة فعالية استهلاك الطاقة","","","","2.93"]
["","عامل الأداء","","","","3.21"]
["","استهلاك الطاقة السنوي","","kWh","","1,024"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","C"]
["","","تدفئة","","","C"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","","A"]
["","الاستطاعة","Pdesign","kW","","6.00"]
["","SEER","","","","5.56"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","378"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","","A"]
["","الاستطاعة","Pdesign","kW","","4.60"]
["","SCOP/A","","","","3.80"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","1,693"]
["Notes","","","","","(1) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","","(2) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["","","","","","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0"]
["","","","","","(4) - تستند استطاعة التدفئة الاسمية إلى: درجة الحرارة الداخلية: 20 درجة مئوية للبويصلة الجافة، درجة الحرارة الخارجية: 7 درجة مئوية للبويصلة الجافة، 6 درجة مئوية للبويصلة الرطبة، الطول المكافئ لمواسير مادة التبريد: 5 متر، فرق المستوى: 0 متر."]
["Outdoor unit","","","","RXM50N2V1B"]
["Cooling capacity","Min.","","kW","1.70"]
["","Nom.","","kW","5.00"]
["","Max.","","kW","5.30"]
["Heating capacity","Min.","","kW","1.70"]
["","Nom.","","kW","5.80"]
["","Max.","","kW","6.00"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","3.06"]
["","عامل الأداء","","","3.10"]
["","استهلاك الطاقة السنوي","","kWh","816"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","B"]
["","","تدفئة","","D"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A+"]
["","الاستطاعة","Pdesign","kW","5.00"]
["","SEER","","","5.77"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","303"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A"]
["","الاستطاعة","Pdesign","kW","4.00"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","3.93"]
["","Pdh استطاعة التدفئة عند -10°","","kW","3.55"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","1424"]
["نطاق كفاءة استخدام الطاقة","","","","A+++ ~ D"]