{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":6,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","","FDXS50F2VEB9"]
["Power input","Cooling","","Nom.","kW","0.060"]
["","Heating","","Nom.","kW","0.060"]
["الأبعاد","الوحدة","","الارتفاع","mm","200"]
["","","","العرض","mm","1150"]
["","","","العمق","mm","620"]
["الوزن","الوحدة","","","kg","30.0"]
["Fan","Air flow rate","Cooling","High","m³/min","12.0"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","11"]
["Fan","Air flow rate","Cooling","Low","m³/min","10.0"]
["","","Heating","High","m³/min","16.0"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","14.8"]
["Fan","Air flow rate","Heating","Low","m³/min","13.5"]
["مروحة","الضغط الاستاتيكي الخارجي","","الإسمي","باسكال","40"]
["مستوى طاقة الصوت","التبريد","","","dBA","55"]
["","التدفئة","","","dBA","55"]
["Sound pressure level","Cooling","","High","dBA","38"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","36"]
["Sound pressure level","Cooling","","Low","dBA","30"]
["","Heating","","High","dBA","38"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","36"]
["Sound pressure level","Heating","","Low","dBA","30"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35"]
["","غاز","","القطر الخارجي","mm","12.7"]
["","التصريف","","","","VP20 (I.D. 20/O.D. 26)"]
["Standard Accessories","دليل التركيب","","","","1"]
["","حلقة للدعامة الحاملة","","","","8"]
["","دليل التشغيل","","","","1"]
["","مشبك معدني","","","","1"]
["","مشابك","","","","6"]
["","خرطوم الصرف","","","","1"]
["","مرشح هواء","","","","1"]
["","عازل لأدوات التثبيت","","","","1"]
["","مسامير لولبية لشفة مجاري الهواء","","","","1"]
["","مواد مانعة للتسريب","","","","2"]
["","لبادة مانعة للتسريب","","","","1"]
["","حلقة للوحة التثبيت","","","","4"]
["وحدة التزويد بالطاقة","الاسم","","","","VE"]
["","الطور","","","","1~"]
["Power supply","Frequency","","","Hz","50/60"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها."]