{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":6,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-B9V / RN-E"]
[]
[]
[]
[]
["","","","","FFQ50B9V1B / RN50E3V1B","FFQ60B9V1B / RN60E3V1B"]
["Cooling capacity","Nom.","","kW","4.70 (3)","5.80 (3)"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","900","1,035"]
["","نسبة فعالية استهلاك الطاقة","","","2.61","2.80"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","D","D"]
["Notes","","","","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)"]
["","","","","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)"]
["","","","","(3) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة‏، 19.0‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية الحوجلة الجافة؛ طول الأنابيب المكافئ: 7.5 م؛ الفرق في المستوى: 0 م","(3) - التبريد: درجة الحرارة الداخلية 27‏° مئوية للحوجلة الجافة‏، 19.0‏° مئوية للحوجلة الرطبة؛ درجة الحرارة الخارجية 35‏° مئوية الحوجلة الجافة؛ طول الأنابيب المكافئ: 7.5 م؛ الفرق في المستوى: 0 م"]
["","","","","(4) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(4) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]