{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":8,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-B9V"]
[]
[]
[]
[]
["","","","","FFQ25B9V1B","FFQ35B9V1B","FFQ50B9V1B","FFQ60B9V1B"]
["Sound pressure level","Cooling","Low","dBA","24.5","25","27","32"]
["","","High","dBA","29.5","32","36","41"]
["Standard Accessories","Operation manual","","","Operation manual","Operation manual","Operation manual","Operation manual"]
["","Installation manual","","","Installation manual","Installation manual","Installation manual","Installation manual"]
["","نموذج ورق للتركيب","","","نموذج ورق للتركيب","نموذج ورق للتركيب","نموذج ورق للتركيب","نموذج ورق للتركيب"]
["","خرطوم الصرف","","","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف","خرطوم الصرف"]
["","مشبك معدني","","","مشبك معدني","مشبك معدني","مشبك معدني","مشبك معدني"]
["","حلقة للوحة التثبيت","","","حلقة للوحة التثبيت","حلقة للوحة التثبيت","حلقة للوحة التثبيت","حلقة للوحة التثبيت"]
["","لباد مانع للتسريب","","","لباد مانع للتسريب","لباد مانع للتسريب","لباد مانع للتسريب","لباد مانع للتسريب"]
["","مشابك","","","مشابك","مشابك","مشابك","مشابك"]
["","مسامير لولبية","","","مسامير لولبية","مسامير لولبية","مسامير لولبية","مسامير لولبية"]
["","حلقة للدعامة الحاملة","","","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة","حلقة للدعامة الحاملة"]
["","عازل لأدوات التثبيت","","","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت","عازل لأدوات التثبيت"]
["Cooling capacity","Total capacity","Nom.","kW","2.5 (1)","3.4 (1)","4.7 (1)","5.8 (1)"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35","6.35","6.35","6.35"]
["","غاز","القطر الخارجي","mm","9.52","9.52","12.7","12.7"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","التبريد","","dBA","46.5","49","53","58"]
["Dimensions","Unit","العرض","mm","575","575","575","575"]
["","","العمق","mm","575","575","575","575"]
["","","الارتفاع","mm","286","286","286","286"]
["الغلاف","المادة","","","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel"]
["","اللون","","","Unpainted","Unpainted","Unpainted","Unpainted"]
["الوزن","الوحدة","","kg","17.5","17.5","17.5","17.5"]
["لوحة ديكور","الوزن","","kg","2.7","2.7","2.7","2.7"]
["","الطراز","","","BYFQ60BW1","BYFQ60BW1","BYFQ60BW1","BYFQ60BW1"]
["","الأبعاد","الارتفاع","mm","55","55","55","55"]
["","","العمق","mm","700","700","700","700"]
["","","العرض","mm","700","700","700","700"]
["","اللون","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["Heating capacity","الاستطاعة الإجمالية","الإسمي","kW","3.2 (2)","4.5 (2)","5.5 (2)","7.0 (2)"]
["Power supply","الطور","","","1~","1~","1~","1~"]
["","Frequency","","Hz","50","50","50","50"]
["","الاسم","","","V1","V1","V1","V1"]
["","Voltage","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m"]
["","","","","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat."]
["","","","","(4) - تعتمد استطاعة التبريد والتدفئة الاسمية على نوع الوحدة الخارجية","(4) - تعتمد استطاعة التبريد والتدفئة الاسمية على نوع الوحدة الخارجية","(4) - تعتمد استطاعة التبريد والتدفئة الاسمية على نوع الوحدة الخارجية","(4) - تعتمد استطاعة التبريد والتدفئة الاسمية على نوع الوحدة الخارجية"]
["","","","","(5) - فئة وحدة PED: Art3§3: مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC","(5) - فئة وحدة PED: Art3§3: مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC","(5) - فئة وحدة PED: Art3§3: مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC","(5) - فئة وحدة PED: Art3§3: مستثنى من مجال PED بسبب المقالة 1، الفقرة 3.6 من ‎97/23/EC"]