{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":9,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-C"]
[]
[]
[]
[]
["","","","","","FFQ25C2VEB","FFQ35C2VEB","FFQ50C2VEB","FFQ60C2VEB"]
["الغلاف","المادة","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["الأبعاد","الوحدة","","الارتفاع","mm","260","260","260","260"]
["","","","العرض","mm","575","575","575","575"]
["","","","العمق","mm","575","575","575","575"]
["الوزن","الوحدة","","","kg","16","16","17.5","17.5"]
["Fan","Air flow rate","Cooling","High","m³/min","9","10","12","14.5"]
["","","","Nom.","m³/min","8","8.5","10","12.5"]
["","","","Low","m³/min","6.5","6.5","7.5","9.5"]
["","","Heating","High","m³/min","9","10","12","14.5"]
["","","","Nom.","m³/min","8","8.5","10","12.5"]
["","","","Low","m³/min","6.5","6.5","7.5","9.5"]
["مستوى طاقة الصوت","التبريد","","","dBA","48","51","56","60"]
["Sound pressure level","Cooling","","High","dBA","31","34","39","43"]
["","","","Nom.","dBA","28.5","30.5","34","40"]
["","","","Low","dBA","25","25","27","32"]
["","Heating","","High","dBA","31","34","39","43"]
["","","","Nom.","dBA","28.5","30.5","34","40"]
["","","","Low","dBA","25","25","27","32"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.52","9.52","12.7","12.7"]
["","التصريف","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["لوحة ديكور","الطراز","","","","BYFQ60CW (لوحة بيضاء)","BYFQ60CW (لوحة بيضاء)","BYFQ60CW (لوحة بيضاء)","BYFQ60CW (لوحة بيضاء)"]
["","اللون","","","","أبيض (N9.5)","أبيض (N9.5)","أبيض (N9.5)","أبيض (N9.5)"]
["","الأبعاد","","الارتفاع","mm","46","46","46","46"]
["","","","العرض","mm","620","620","620","620"]
["","","","العمق","mm","620","620","620","620"]
["","الوزن","","","kg","2.8","2.8","2.8","2.8"]
["لوحة ديكور 2","الطراز","","","","BYFQ60CS (لوحة رمادية)","BYFQ60CS (لوحة رمادية)","BYFQ60CS (لوحة رمادية)","BYFQ60CS (لوحة رمادية)"]
["","اللون","","","","أبيض (N9.5) + فضي","أبيض (N9.5) + فضي","أبيض (N9.5) + فضي","أبيض (N9.5) + فضي"]
["","الأبعاد","","الارتفاع","mm","46","46","46","46"]
["","","","العرض","mm","620","620","620","620"]
["","","","العمق","mm","620","620","620","620"]
["","الوزن","","","kg","2.8","2.8","2.8","2.8"]
["لوحة ديكور 3","الطراز","","","","BYFQ60B3W1 (لوحة قياسية)","BYFQ60B3W1 (لوحة قياسية)","BYFQ60B3W1 (لوحة قياسية)","BYFQ60B3W1 (لوحة قياسية)"]
["","اللون","","","","أبيض (RAL9010)","أبيض (RAL9010)","أبيض (RAL9010)","أبيض (RAL9010)"]
["","الأبعاد","","الارتفاع","mm","55","55","55","55"]
["","","","العرض","mm","700","700","700","700"]
["","","","العمق","mm","700","700","700","700"]
["","الوزن","","","kg","2.7","2.7","2.7","2.7"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","BRC7F530W (لوحة بيضاء), BRC7F530S (لوحة رمادية), BRC7EB530 (لوحة قياسية)","BRC7F530W (لوحة بيضاء), BRC7F530S (لوحة رمادية), BRC7EB530 (لوحة قياسية)","BRC7F530W (لوحة بيضاء), BRC7F530S (لوحة رمادية), BRC7EB530 (لوحة قياسية)","BRC7F530W (لوحة بيضاء), BRC7F530S (لوحة رمادية), BRC7EB530 (لوحة قياسية)"]
["","جهاز تحكم عن بُعد سلكي","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Standard Accessories","دليل التركيب","","","","1","1","1","1"]
["","حلقة للدعامة الحاملة","","","","8","8","8","8"]
["","دليل التشغيل","","","","1","1","1","1"]
["","مشابك","","","","7","7","7","7"]
["","خرطوم الصرف","","","","1","1","1","1"]
["","عازل لأدوات التثبيت","","","","2","2","2","2"]
["","مشبك معدني لخرطوم الصرف","","","","1","1","1","1"]
["","نموذج ورق للتركيب","","","","1","1","1","1"]
["","مسامير لولبية","","","","4","4","4","4"]
["","لبادة مانعة للتسريب","","","","4","4","4","4"]
["وحدة التزويد بالطاقة","الاسم","","","","VE","VE","VE","VE"]
["","الطور","","","","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - الأبعاد لا تشمل علبة التحكم","(1) - الأبعاد لا تشمل علبة التحكم","(1) - الأبعاد لا تشمل علبة التحكم","(1) - الأبعاد لا تشمل علبة التحكم"]
["","","","","","(2) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(2) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(2) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(2) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت."]