{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":9,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A"]
[]
[]
[]
[]
["","","","","","FHA35AVEB","FHA50AVEB","FHA60AVEB","FHA71AVEB"]
["الغلاف","اللون","","","","أبيض","أبيض","أبيض","أبيض"]
["","المادة","","","","راتنج، صفائح معدنية","راتنج، صفائح معدنية","راتنج، صفائح معدنية","راتنج، صفائح معدنية"]
["الأبعاد","الوحدة","","الارتفاع","mm","235","235","235","235"]
["","","","العرض","mm","960","960","1270","1270"]
["","","","العمق","mm","690","690","690","690"]
["الوزن","الوحدة","","","kg","24.0","25.0","31.0","32.0"]
["Fan","Air flow rate","Cooling","High","m³/min","14.0","15.0","19.5","20.5"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","11.5","12.0","15.0","17.0"]
["Fan","Air flow rate","Cooling","Low","m³/min","10.0","10.0","11.5","14.0"]
["","","Heating","High","m³/min","14.0","15.0","19.5","20.5"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","11.5","12.0","15.0","17.0"]
["Fan","Air flow rate","Heating","Low","m³/min","10.0","10.0","11.5","14.0"]
["مستوى طاقة الصوت","التبريد","","","dBA","53","54","54","55"]
["Sound pressure level","Cooling","","High","dBA","36","37","37","38"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","34","35","35","36"]
["Sound pressure level","Cooling","","Low","dBA","31","32","33","34"]
["","Heating","","High","dBA","36","37","37","38"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","31","32","33","34"]
["Sound pressure level","Heating","","Nom.","dBA","34","35","35","36"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35","9.52"]
["","غاز","","القطر الخارجي","mm","9.50","12.7","12.7","15.9"]
["","التصريف","","","","VP20","VP20","VP20","VP20"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56"]
["","جهاز تحكم عن بُعد سلكي","","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["Standard Accessories","أنبوب العزل الحراري","","","","2","2","2","2"]
["","تثبيت بالراتنج","","","","1","1","1","1"]
["","مثبتات الأسلاك","","","","2","2","2","2"]
["","حلقة تثبيت الخرطوم","","","","1","1","1","1"]
["","مادة مشبك السلك","","","","7","7","7","7"]
["","خرطوم الصرف","","","","1","1","1","1"]
["","مسامير لولبية","","","","2","2","2","2"]
["","لبادة مانعة للتسريب (كبيرة)","","","","1","1","1","1"]
["","لبادة مانعة للتسريب (صغيرة)","","","","1","1","1","1"]
["","حلقة إحكام الربط","","","","8","8","8","8"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]