{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-B8 / RKS-J"]
[]
[]
[]
[]
["","","","","FHQ35BWV1B / RKS35J2V1B","FHQ50BWV1B / RKS50J2V1B"]
["Cooling capacity","Min.","","kW","1.4","1.7"]
["","Max.","","kW","3.7","5.6"]
["","Nom.","","kW","3.4 (3)","5.0 (3)"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35","6.35"]
["","غاز","القطر الخارجي","mm","9.5","12.7"]
["","Drain","OD","mm","VP20 (القطر الخارجي 26؛ القطر الداخلي 20)","VP20 (القطر الخارجي 26؛ القطر الداخلي 20)"]
["Notes","","","","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)"]
["","","","","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(4) - SL: The silent fan level of the air flow rate setting","(4) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected."]
["","","","","(5) - 220 فولت"]
["","","","","(6) - 230 فولت"]
["","","","","(7) - 240 فولت"]