{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-B8 / RXS-F"]
[]
[]
[]
[]
["","","","","FHQ60BWV1B / RXS60F3V1B"]
["Cooling capacity","Min.","","kW","1.7"]
["","Max.","","kW","6.0"]
["","Nom.","","kW","5.7 (3)"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35"]
["","غاز","القطر الخارجي","mm","12.7"]
["","Drain","OD","mm","VP20 (القطر الخارجي 26؛ القطر الداخلي 20)"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","1,075"]
["","نسبة فعالية استهلاك الطاقة","","","2.65"]
["","عامل الأداء","","","2.89"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","D"]
["","","تدفئة","","D"]
["Heating capacity","Nom.","","kW","7.2 (4)"]
["","Min.","","kW","1.7"]
["","Max.","","kW","8.0"]
["Notes","","","","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)"]
["","","","","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(5) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]