{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":12,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-CB"]
[]
[]
[]
[]
["","","","","","FHQ35CBVEB","FHQ50CBVEB","FHQ60CBVEB","FHQ71CBVEB","FHQ100CBVEB","FHQ125CBVEB","FHQ140CBVEB"]
["الغلاف","اللون","","","","أبيض","أبيض","أبيض","أبيض","أبيض","أبيض","أبيض"]
["","المادة","","","","راتنج، صفائح معدنية","راتنج، صفائح معدنية","راتنج، صفائح معدنية","راتنج، صفائح معدنية","راتنج، صفائح معدنية","راتنج، صفائح معدنية","راتنج، صفائح معدنية"]
["الأبعاد","الوحدة","","الارتفاع","mm","235","235","235","235","235","235","235"]
["","","","العرض","mm","960","960","1270","1270","1590","1590","1590"]
["","","","العمق","mm","690","690","690","690","690","690","690"]
["الوزن","الوحدة","","","kg","24","25","31","32","38","38","38"]
["Fan","Air flow rate","Cooling","High","m³/min","14","15","19.5","20.5","28","31","34"]
["","","","Nom.","m³/min","11.5","12","15","17","24","27","29"]
["","","","Low","m³/min","10","10","11.5","14","20","23","24"]
["","","Heating","High","m³/min","14","15","19.5","20.5","28","31","34"]
["","","","Nom.","m³/min","11.5","12","15","17","24","27","29"]
["","","","Low","m³/min","10","10","11.5","14","20","23","24"]
["مستوى طاقة الصوت","التبريد","","","dBA","53","54","54","55","60","62","64"]
["","التدفئة","","","dBA","53","54","54","55","60","62","64"]
["Sound pressure level","Cooling","","High","dBA","36","37","37","38","42","44","46"]
["","","","Nom.","dBA","34","35","35","36","38","41","42"]
["","","","Low","dBA","31","32","33","34","34","37","38"]
["","Heating","","High","dBA","36","37","37","38","42","44","46"]
["","","","Nom.","dBA","34","35","35","36","38","41","42"]
["","","","Low","dBA","31","32","33","34","34","37","38"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","غاز","","القطر الخارجي","mm","9.5","12.7","12.7","15.9","15.9","15.9","15.9"]
["","التصريف","","","","VP20","VP20","VP20","VP20","VP20","VP20","VP20"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53"]
["","جهاز تحكم عن بُعد سلكي","","","","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A"]
["وحدة التزويد بالطاقة","الطور","","","","1~","1~","1~","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]