{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":8,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQG-C"]
[]
[]
[]
[]
["","","","","FHQG71CVEB","FHQG100CVEB","FHQG125CVEB","FHQG140CVEB"]
["Sound pressure level","Heating","High","dBA","38","42","44","46"]
["","","Nom.","dBA","36","38","41","42"]
["","","Low","dBA","34","34","37","38"]
["","Cooling","Low","dBA","34","34","37","38"]
["","","High","dBA","38","42","44","46"]
["","","Nom.","dBA","36","38","41","42"]
["Piping connections","Liquid","القطر الخارجي","mm","9.52","9.52","9.52","9.52"]
["","غاز","القطر الخارجي","mm","15.9","15.9","15.9","15.9"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","التبريد","","dBA","55","60","62","64"]
["Dimensions","Unit","العرض","mm","1,270","1,590","1,590","1,590"]
["","","العمق","mm","690","690","690","690"]
["","","الارتفاع","mm","235","235","235","235"]
["الغلاف","اللون","","","أبيض صاف","أبيض صاف","أبيض صاف","أبيض صاف"]
["الوزن","الوحدة","","kg","32","38","38","38"]
["Power supply","الطور","","","1~","1~","1~","1~"]
["","Frequency","","Hz","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240"]