{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":8,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B / RXS-K"]
[]
[]
[]
[]
["","","","","FLXS25BAVMB / RXS25K3V1B","FLXS25BAVMB / RXS25K2V1B","FLXS35BAVMB / RXS35K2V1B","FLXS50BAVMB / RXS50K2V1B"]
["Cooling capacity","Min.","","kW","1.2","1.2","1.2","0.9"]
["","Max.","","kW","3.0","3.0","3.8","5.3"]
["","Nom.","","kW","2.5 (2)","2.5 (3)","3.5 (2)","4.9 (2)"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35","6.35","6.35","6.35"]
["","غاز","القطر الخارجي","mm","9.5","9.5","9.5","12.7"]
["","Drain","OD","mm","18.0","18","18.0","18.0"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","325","325","565","860"]
["","نسبة فعالية استهلاك الطاقة","","","3.85","3.85","3.10","2.85"]
["","عامل الأداء","","","3.47","3.47","3.25","3.35"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","B","C"]
["","","تدفئة","","B","B","C","C"]
["Heating capacity","Nom.","","kW","3.4 (3)","3.4 (4)","4.0 (3)","6.1 (3)"]
["","Min.","","kW","1.2","1.2","1.4","0.9"]
["","Max.","","kW","4.5","4.5","5.0","7.5"]
["Notes","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(4) - 220 فولت","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(4) - 220 فولت","(4) - 220 فولت"]
["","","","","(5) - 230 فولت","(5) - 220 فولت","(5) - 230 فولت","(5) - 230 فولت"]
["","","","","(6) - 240 فولت","(6) - 230 فولت","(6) - 240 فولت","(6) - 240 فولت"]
["","","","","(7) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(7) - 240 فولت","(7) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(7) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]
["","","","","","(8) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]