{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":6,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","","FLXS35BAVMB9"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","7.6"]
["Sound pressure level","Cooling","","Nom.","dBA","35"]
["Fan","Air flow rate","Heating","Nom.","m³/min","10.4"]
["Sound pressure level","Heating","","Nom.","dBA","36"]
["الغلاف","اللون","","","","Almond white"]
["الأبعاد","الوحدة","","الارتفاع","mm","490"]
["","","","العرض","mm","1050"]
["","","","العمق","mm","200"]
["الوزن","الوحدة","","","kg","16"]
["Fan","Air flow rate","Cooling","High","m³/min","8.6"]
["","","","Low","m³/min","6.6"]
["","","","Silent operation","m³/min","5.6"]
["","","Heating","High","m³/min","12.8"]
["","","","Low","m³/min","8"]
["","","","Silent operation","m³/min","7.2"]
["مستوى طاقة الصوت","التبريد","","","dBA","53"]
["","التدفئة","","","dBA","59"]
["Sound pressure level","Cooling","","High","dBA","38"]
["","","","Low","dBA","32"]
["","","","Silent operation","dBA","29"]
["","Heating","","High","dBA","46"]
["","","","Low","dBA","33"]
["","","","Silent operation","dBA","30"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35"]
["","غاز","","القطر الخارجي","mm","9.5"]
["","التصريف","","","","18"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","ARC433B67"]
["Standard Accessories","دليل التركيب","","","","1"]
["","مرشح تنقية الهواء","","","","1"]
["","بطاريات جافة قياس AAA","","","","2"]
["","رباط تحزيم","","","","4"]
["","دليل التشغيل","","","","1"]
["","أنبوب عزل الحرارة (أنبوب سائل التبريد)","","","","8"]
["","جهاز تحكم عن بعد بالأشعة تحت الحمراء","","","","1"]
["","لوح التثبيت","","","","1"]
["","مرشح إزالة الروائح بالتحفيز الضوئي","","","","1"]
["","حامل جهاز التحكم عن بعد","","","","1"]
["","غطاء جانبي","","","","2"]
["وحدة التزويد بالطاقة","الاسم","","","","VM"]
["","الطور","","","","1~"]
["Power supply","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - 220 فولت"]
["","","","","","(2) - 230 فولت"]
["","","","","","(3) - 240 فولت"]
["","","","","","(4) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها."]