{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FNA25A2VEB / RXM25M3V1B9","FNA35A2VEB / RXM35M3V1B9","FNA50A2VEB / RXM50M3V1B9","FNA60A2VEB / RXM60M3V1B9"]
["Cooling capacity","Nom.","","kW","2.60","3.40","5.00","6.00"]
["تبريد المساحة","SEER","","","5.68","5.70","5.77","5.56"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","160","209","303","378"]
["","الاستطاعة","Pdesign","kW","2.60","3.40","5.00","6.00"]
["","فئة فعالية استهلاك الطاقة","","","A+","A+","A+","A"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","2.80","2.90","4.00","4.60"]
["","SCOP/A","","","4.24","4.05","4.09","4.16"]
["","فئة فعالية استهلاك الطاقة","","","A+","A+","A+","A+"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","924","1,002","1,369","1,547"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","342","551","739","1,111"]
["","نسبة فعالية استهلاك الطاقة","","","3.80","3.09","3.38","2.70"]
["","عامل الأداء","","","4.00","3.48","3.34","3.11"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","B","A","D"]
["","","تدفئة","","A","B","C","D"]
["Heating capacity","Nom.","","kW","3.20","4.00","5.80","7.00"]
["Notes","","","","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - انظر الرسم المنفصل لنطاق التشغيل","(1) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","(2) - انظر الرسم المنفصل لنطاق التشغيل","(2) - انظر الرسم المنفصل لنطاق التشغيل","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0"]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]