{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":9,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FNA50A2VEB / FNA50A2VEB / RZQSG100L8Y1B","FNA35A2VEB / FNA35A2VEB / FNA35A2VEB / RZQSG100L8Y1B","FNA50A2VEB / FNA50A2VEB / FNA50A2VEB / RZQSG125L8Y1B","FNA60A2VEB / FNA60A2VEB / RZQSG125L8Y1B","FNA35A2VEB / FNA35A2VEB / FNA35A2VEB / FNA35A2VEB / RZQSG125L8Y1B"]
["Cooling capacity","Nom.","","kW","9.50 (1)","9.50 (1)","12.0 (1)","12.0 (1)","12.0 (1)"]
["تبريد المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","652","693","875","875","875"]
["","الاستطاعة","Pdesign","kW","9.50","9.50","12.0","12.0","12.0"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","7.60","7.10","7.60","7.60","7.60"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","2,800","2,616","2,800","2,800","2,800"]
["الفعالية الاسمية","نسبة فعالية استهلاك الطاقة","","","3.02 (3)","2.56 (3)","2.95 (3)","2.46 (3)","2.57 (3)"]
["","عامل الأداء","","","3.26 (3)","2.66 (3)","3.44 (3)","3.08 (3)","2.90 (3)"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","B","E","C","E","E"]
["","","تدفئة","","C","D","B","D","D"]
["Heating capacity","Nom.","","kW","10.8 (2)","10.8 (2)","13.5 (2)","13.5 (2)","13.5 (2)"]
["تبريد المساحة","SEER","","","5.10","4.80","4.80","4.80","4.80"]
["","فئة فعالية استهلاك الطاقة","","","A","B","B","B","B"]
["تدفئة المساحة (مناخ معتدل)","SCOP/A","","","3.80","3.80","3.80","3.80","3.80"]
["","فئة فعالية استهلاك الطاقة","","","A","A","A","A","A"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(3) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]