{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":9,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A"]
[]
[]
[]
[]
["","","","","","FNA25A2VEB","FNA35A2VEB","FNA50A2VEB","FNA60A2VEB"]
["مروحة","الضغط الاستاتيكي الخارجي","","عالٍ","باسكال","48","48","49","49"]
["الغلاف","اللون","","","","Unpainted","Unpainted","Unpainted","Unpainted"]
["","المادة","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["الأبعاد","الوحدة","","الارتفاع","mm","620, 720 (2) (1), 720 (2) (1)","620, 720 (1) (2), 720 (1) (2)","620, 720 (2) (1), 720 (2) (1)","620, 720 (2) (1), 720 (2) (1)"]
["","","","العرض","mm","790","790","1190","1190"]
["","","","العمق","mm","200","200","200","200"]
["الوزن","الوحدة","","","kg","23","23","30","30"]
["Fan","Air flow rate","Cooling","High","m³/min","8.7","8.7","16","16"]
["","","","Nom.","m³/min","8","8","14.8","14.8"]
["","","","Low","m³/min","7.3","7.3","13.5","13.5"]
["","","Heating","High","m³/min","8.7","8.7","16","16"]
["","","","Nom.","m³/min","8","8","14.8","14.8"]
["","","","Low","m³/min","7.3","7.3","13.5","13.5"]
["مروحة","الضغط الاستاتيكي الخارجي","","الإسمي","باسكال","30","30","40","40"]
["مستوى طاقة الصوت","التبريد","","","dBA","53","53","56","56"]
["Sound pressure level","Cooling","","High","dBA","33","33","36","36"]
["","","","Nom.","dBA","31","31","33","33"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","31","31","33","33"]
["Sound pressure level","Cooling","","Low","dBA","28","28","30","30"]
["","Heating","","High","dBA","33","33","36","36"]
["","","","Nom.","dBA","31","31","33","33"]
["","","","Low","dBA","28","28","30","30"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.52","9.52","12.7","12.7"]
["","التصريف","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["","جهاز تحكم عن بُعد سلكي","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["وحدة التزويد بالطاقة","الاسم","","","","VE","VE","VE","VE"]
["","الطور","","","","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50/60","50/60","50/60","50/60"]
["","Voltage","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","","(1) - يتضمن أرجل التركيب","(1) - يتضمن أرجل التركيب","(1) - يتضمن أرجل التركيب","(1) - يتضمن أرجل التركيب"]
["","","","","","(2) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(2) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(2) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت.","(2) - مستوى قوة الصوت هو قيمة مطلقة تشير إلى الطاقة التي يولدها مصدر الصوت."]