{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTN-F / RN-E"]
[]
[]
[]
[]
["","","","","FTN50FV1B / RN50E3V1B","FTN60FV1B / RN60E3V1B"]
["Cooling capacity","Nom.","","kW","5.0 (3)","6.0 (3)"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35","6.35"]
["","غاز","القطر الخارجي","mm","12.7","12.7"]
["","Drain","OD","mm","18.0","18.0"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","775","995"]
["","نسبة فعالية استهلاك الطاقة","","","3.23","3.02"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","B"]
["Notes","","","","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)"]
["","","","","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 7°CDB, 6°CWB; equivalent piping length: 7.5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 7°CDB, 6°CWB; equivalent piping length: 7.5m"]
["","","","","(4) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(4) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]