{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTN-F"]
[]
[]
[]
[]
["","","","","","FTN50FV1B","FTN60FV1B"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","12.4","13.6"]
["الغلاف","اللون","","","","أبيض","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","290","290"]
["","","","العرض","mm","1050","1050"]
["","","","العمق","mm","238","238"]
["الوزن","الوحدة","","","kg","12","12"]
["Fan","Air flow rate","Cooling","High","m³/min","14.7","16.2"]
["","","","Low","m³/min","10.3","11.4"]
["مستوى طاقة الصوت","التبريد","","","dBA","59","61"]
["Sound pressure level","Cooling","","High","dBA","43","45"]
["","","","Low","dBA","34","36"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","12.7","12.7"]
["","التصريف","","","","18","18"]
["Standard Accessories","دليل التركيب","","","","1","1"]
["","جهاز تحكم عن بعد لاسلكي","","","","1","1"]
["","دليل التشغيل","","","","1","1"]
["","البطاريات","","","","2","2"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","","2","2"]
["","لوح التثبيت","","","","1","1"]
["","حامل جهاز التحكم عن بعد","","","","1"]
["","مرشح تنقية الهواء بالتحفيز الضوئي وأباتيت التيتانيوم","","","","2","2"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1"]
["","الطور","","","","1~","1~"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]