{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":11,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-GV"]
[]
[]
[]
[]
["","","","","","FTX20GV1B","FTX25GV1B","FTX35GV1B","FTX50GV1B","FTX60GV1B","FTX71GV1B"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","7.4","7.6","7.7","14.7","16.2","14.6"]
["Sound pressure level","Cooling","","Nom.","dBA","33","33","34","39","41","42"]
["Fan","Air flow rate","Heating","Nom.","m³/min","7.8","8.0","8.4","13.9","15.1","16.9"]
["Sound pressure level","Heating","","Nom.","dBA","34","34","35","38","40","42"]
["Power input","Cooling","","Nom.","kW","","","","0.034","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["","Heating","","Nom.","kW","","","","0.036","0.045 (3) (4) (2), 0.045 (3) (4) (2), 0.045 (3) (4) (2)","0.060 (3) (2), 0.060 (3) (2), 0.06 (4)"]
["الغلاف","اللون","","","","أبيض","أبيض","أبيض","أبيض","أبيض","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","283","283","283","290","290","290"]
["","","","العرض","mm","770","770","770","1050","1050","1050"]
["","","","العمق","mm","198","198","198","238","238","238"]
["الوزن","الوحدة","","","kg","7","7","7","12","12","12"]
["Fan","Air flow rate","Cooling","High","m³/min","9.1","9.2","9.3","14.7","16.2","17.4"]
["","","","Low","m³/min","5.9","6.0","6.1","10.3","11.4","11.6"]
["","","","Silent operation","m³/min","4.7","4.8","4.9","9.5","10.2","10.6"]
["","","Heating","High","m³/min","9.4","9.7","10.1","16.1","17.4","19.7"]
["","","","Low","m³/min","6.3","6.3","6.7","11.5","12.7","14.3"]
["","","","Silent operation","m³/min","5.5","5.5","5.7","10.2","11.4","12.7"]
["مستوى طاقة الصوت","التبريد","","","dBA","55","56","57","59","60","63"]
["","التدفئة","","","dBA","55","56","57","58","59","62"]
["Sound pressure level","Cooling","","High","dBA","39","40","41","43","45","46"]
["","","","Low","dBA","25","26","27","34","36","37"]
["","","","Silent operation","dBA","22","22","23","31","33","34"]
["","Heating","","High","dBA","39","40","41","42","44","46"]
["","","","Low","dBA","28","28","29","33","35","37"]
["","","","Silent operation","dBA","25","25","26","30","32","34"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.52","9.52","9.52","12.7","12.7","15.9"]
["","التصريف","","","","18","18","18","18","18","18"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","","","","ARC433B70","ARC433B70","ARC433B70"]
["Standard Accessories","دليل التركيب","","","","1","1","1","1","1","1"]
["","جهاز تحكم عن بعد لاسلكي","","","","1","1","1","1","1","1"]
["","دليل التشغيل","","","","1","1","1","1","1","1"]
["","البطاريات","","","","2","2","2","2","2","2"]
["","مسمار تثبيت لولبي للوحدة الداخلية","","","","2","2","2"]
["","لوح التثبيت","","","","1","1","1","1","1","1"]
["","حامل جهاز التحكم عن بعد","","","","1","1","1","1","1","1"]
["","مرشح تنقية الهواء بالتحفيز الضوئي وأباتيت التيتانيوم","","","","2","2","2","2","2","2"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1","V1","V1","V1","V1"]
["","الطور","","","","1~","1~","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standard Accessories","مسامير لولبية لتثبيت الوحدة الداخلية","","","","","","","2","2"]
["Notes","","","","","","","","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء"]
["","","","","","","","","(2) - 220 فولت","(2) - 220 فولت","(2) - 220 فولت"]
["","","","","","","","","(3) - 230 فولت","(3) - 230 فولت","(3) - 230 فولت"]
["","","","","","","","","(4) - 240 فولت","(4) - 240 فولت","(4) - 240 فولت"]
["Standard Accessories","براغي تثبيت الوحدة الداخلية (M4 x 12L)","","","","","","","","","2"]