{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-J3"]
[]
[]
[]
[]
["","","","","","FTX20J3V1B","FTX25J3V1B","FTX35J3V1B"]
["Power input","Cooling","","Nom.","kW","0.03","0.030","0.030"]
["","Heating","","Nom.","kW","0.04","0.040","0.040"]
["الغلاف","اللون","","","","أبيض","أبيض","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","198","198","198"]
["","","","العرض","mm","770","770","770"]
["","","","العمق","mm","283","283","283"]
["الوزن","الوحدة","","","kg","7","7.00","7.00"]
["Fan","Air flow rate","Cooling","High","m³/min","9.1","9.2","9.3"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","7.4","7.6","7.7"]
["Fan","Air flow rate","Cooling","Low","m³/min","5.9","6.0","6.1"]
["","","","Silent operation","m³/min","4.7","4.8","4.9"]
["","","Heating","High","m³/min","9.4","9.7","10.1"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","7.8","8.0","8.4"]
["Fan","Air flow rate","Heating","Low","m³/min","6.3","6.3","6.7"]
["","","","Silent operation","m³/min","5.5","5.5","5.7"]
["مستوى طاقة الصوت","التبريد","","","dBA","55","55","58"]
["","التدفئة","","","dBA","55","55","58"]
["Sound pressure level","Cooling","","High","dBA","39","40","41"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","33","33","34"]
["Sound pressure level","Cooling","","Low","dBA","25","26","27"]
["","","","Silent operation","dBA","22","22","23"]
["","Heating","","High","dBA","39","40","41"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","34","34","35"]
["Sound pressure level","Heating","","Low","dBA","28","28","29"]
["","","","Silent operation","dBA","25","25","26"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.5","9.50","9.50"]
["","التصريف","","","","18","18","18"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","ARC433A87","ARC433A87","ARC433A87"]
["Standard Accessories","دليل التركيب","","","","1","1","1"]
["","جهاز تحكم عن بعد لاسلكي","","","","1","1","1"]
["","بطاريات جافة قياس AAA","","","","2","2","2"]
["","دليل التشغيل","","","","1","1","1"]
["","مرشح أباتيت التيتانيوم المزيل للروائح","","","","2","2","2"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","","2","2","2"]
["","لوح التثبيت","","","","1","1","1"]
["","حامل جهاز التحكم عن بعد","","","","1","1","1"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1","V1"]
["","الطور","","","","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]