{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":10,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-K"]
[]
[]
[]
[]
["","","","","","FTX20KV1B","FTX25KV1B","FTX35KV1B","FTX50KV1B","FTX60KV1B"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","7.8","8.0","8.2","13.7","14.9"]
["Sound pressure level","Cooling","","Nom.","dBA","33","33","34","39","41"]
["Fan","Air flow rate","Heating","Nom.","m³/min","8.5","8.5","8.5","14.7","16.7"]
["Sound pressure level","Heating","","Nom.","dBA","34","34","35","38","40"]
["الغلاف","اللون","","","","أبيض","أبيض","أبيض","أبيض","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","286","286","286","295","295"]
["","","","العرض","mm","770","770","770","990","990"]
["","","","العمق","mm","225","225","225","263","263"]
["الوزن","الوحدة","","","kg","8","8","8","12","12"]
["Fan","Air flow rate","Cooling","High","m³/min","9.9","10.4","11.8","16","17.6"]
["","","","Low","m³/min","5.8","6.1","6.3","11.1","12.2"]
["","","","Silent operation","m³/min","4.8","4.8","4.9","10.1","11.2"]
["","","Heating","High","m³/min","10.9","11.1","12.8","16.7","18.9"]
["","","","Low","m³/min","6.4","6.7","6.9","12.2","13.7"]
["","","","Silent operation","m³/min","5.2","5.2","5.2","10.9","12.1"]
["مستوى طاقة الصوت","التبريد","","","dBA","55","55","58","59","60"]
["","التدفئة","","","dBA","55","55","58","58","59"]
["Sound pressure level","Cooling","","High","dBA","39","40","43","43","45"]
["","","","Low","dBA","25","26","27","34","36"]
["","","","Silent operation","dBA","20","20","20","31","33"]
["","Heating","","High","dBA","39","40","43","42","44"]
["","","","Low","dBA","28","28","29","33","35"]
["","","","Silent operation","dBA","23","23","26","30","32"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.5","9.5","9.5","12.7","12.7"]
["","التصريف","","","","18","18","18","16","16"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11"]
["","جهاز تحكم عن بُعد سلكي","","","","BRC073, BRC944B2","BRC073, BRC944B2","BRC073, BRC944B2","BRC073, BRC944B2","BRC073, BRC944B2"]
["Standard Accessories","دليل التركيب","","","","1","1","1","1","1"]
["","بطاريات جافة قياس AA","","","","2","2","2","2","2"]
["","دليل التشغيل","","","","1","1","1","1","1"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","","2","2","2","2","2"]
["","جهاز تحكم عن بعد بالأشعة تحت الحمراء","","","","1","1","1","1","1"]
["","لوح التثبيت","","","","1","1","1","1","1"]
["","حامل جهاز التحكم عن بعد","","","","1","1","1","1","1"]
["","مرشح تنقية الهواء بالتحفيز الضوئي وأباتيت التيتانيوم","","","","2","2","2","2","2"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1","V1","V1","V1"]
["","الطور","","","","1~","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240"]