{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":14,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-KV"]
[]
[]
[]
[]
["","","","","","FTX20K2V1B","FTX20K5V1B","FTX25K2V1B","FTX25K5V1B","FTX35K2V1B","FTX35K5V1B","FTX50K2V1B","FTX60K2V1B","FTX71K2V1B"]
["Power input","Cooling","","Nom.","kW","0.018","0.018","0.02","0.02","0.024","0.024","0.035","0.041","0.041"]
["","Heating","","Nom.","kW","0.022","0.022","0.023","0.023","0.029","0.029","0.038","0.044","0.044"]
["الغلاف","اللون","","","","أبيض","أبيض","أبيض","أبيض","أبيض","أبيض","أبيض","أبيض","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","286","286","286","286","286","286","295","295","295"]
["","","","العرض","mm","770","770","770","770","770","770","990","990","990"]
["","","","العمق","mm","225","225","225","225","225","225","263","263","263"]
["الوزن","الوحدة","","","kg","8.5","8.5","8.5","8.5","9","9","13.5","13.5","13.5"]
["Fan","Air flow rate","Cooling","High","m³/min","9.9","9.9","10.4","10.4","11.8","11.8","16","17.6","17.6"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","7.8","7.8","8","8","8.2","8.2","13.7","14.9","14.9"]
["Fan","Air flow rate","Cooling","Low","m³/min","5.8","5.8","6.1","6.1","6.3","6.3","11.1","12.2","12.2"]
["","","","Silent operation","m³/min","4.8","4.8","4.8","4.8","4.9","4.9","10.1","11.2","11.2"]
["","","Heating","High","m³/min","10.9","10.9","11.1","11.1","12.8","12.8","16.7","18.9","18.9"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","8.5","8.5","8.5","8.5","8.5","8.5","14.7","16.7","16.7"]
["Fan","Air flow rate","Heating","Low","m³/min","6.4","6.4","6.7","6.7","6.9","6.9","12.2","13.7","13.7"]
["","","","Silent operation","m³/min","5.2","5.2","5.2","5.2","5.2","5.2","10.9","12.1","12.1"]
["مستوى طاقة الصوت","التبريد","","","dBA","55","55","55","55","58","58","59","60","62"]
["","التدفئة","","","dBA","55","55","55","55","58","58","58","59","61"]
["Sound pressure level","Cooling","","High","dBA","39","39","40","40","43","43","43","45","46"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","33","33","33","33","34","34","39","41","42"]
["Sound pressure level","Cooling","","Low","dBA","25","25","26","26","27","27","34","36","37"]
["","","","Silent operation","dBA","20","20","20","20","20","20","31","33","34"]
["","Heating","","High","dBA","39","39","40","40","43","43","42","44","45"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","34","34","34","34","35","35","38","40","41"]
["Sound pressure level","Heating","","Low","dBA","28","28","28","28","29","29","33","35","36"]
["","","","Silent operation","dBA","23","23","23","23","26","26","30","32","33"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.5","9.5","9.5","9.5","9.5","9.5","12.7","12.7","12.7"]
["","التصريف","","","","18","18","18","18","18","18","16","16","16"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11"]
["","جهاز تحكم عن بُعد سلكي","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073","BRC944B2, BRC073","BRC944B2, BRC073"]
["Standard Accessories","دليل التركيب","","","","1","1","1","1","1","1","1","1","1"]
["","بطاريات جافة قياس AAA","","","","2","2","2","2","2","2","2","2","2"]
["","دليل التشغيل","","","","1","1","1","1","1","1","1","1","1"]
["","مرشح أباتيت التيتانيوم المزيل للروائح","","","","2","2","2","2","2","2","2","2","2"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","","2","2","2","2","2","2","2","2","2"]
["","جهاز تحكم عن بعد بالأشعة تحت الحمراء","","","","1","1","1","1","1","1","1","1","1"]
["","لوح التثبيت","","","","1","1","1","1","1","1","1","1","1"]
["","حامل جهاز التحكم عن بعد","","","","1","1","1","1","1","1","1","1","1"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1","V1","V1","V1","V1"]
["","الطور","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","","","","","","","","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]