{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":57,"n_cols":11,"rows_kept":57,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXB-B"]
[]
[]
[]
[]
["","","","","","FTXB50BV1B","FTXB25B1V1","FTXB25BV1","FTXB35B1V1","FTXB35BV1","FTXB60BV1B"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","13.32","7.6","7.4","7.7","7.6","16.56"]
["Sound pressure level","Cooling","","Nom.","dBA","38","33","33","34","34","41"]
["Fan","Air flow rate","Heating","Nom.","m³/min","13.32","8.0","","8.4","8.0","16.56"]
["Sound pressure level","Heating","","Nom.","dBA","38","33","33","34","34","41"]
["Power input","Cooling","","Nom.","kW","","0.030","0.040","0.030","0.040"]
["","Heating","","Nom.","kW","","0.040","0.040","0.040","0.040"]
["الغلاف","اللون","","","","أبيض","","","","","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","310","283","283","283","283","310"]
["","","","العرض","mm","1065","770","770","770","770","1065"]
["","","","العمق","mm","224","216","216","216","216","224"]
["الوزن","الوحدة","","","kg","14","7","8","7","8","14"]
["Fan","Air flow rate","Cooling","High","m³/min","15.00","9.2","9.0","9.3","9.2","18.54"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","","7.6","","7.7"]
["Fan","Air flow rate","Cooling","Low","m³/min","11.82","6.0","5.8","6.1","6.0","14.34"]
["","","","Silent operation","m³/min","10.62","4.8","4.6","4.9","4.8","12.36"]
["","","Heating","High","m³/min","15.00","9.7","9.5","10.1","9.7","18.54"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","","8.0","","8.4"]
["Fan","Air flow rate","Heating","Low","m³/min","11.82","6.3","","6.7","6.3","14.34"]
["","","","Silent operation","m³/min","10.62","5.5","","5.7","5.5","12.36"]
["مستوى طاقة الصوت","التبريد","","","dBA","55","52","52","53","53","61"]
["","التدفئة","","","dBA","","52","52","54","54"]
["Sound pressure level","Cooling","","Super high","dBA","44","","","","","46"]
["","","","High","dBA","40","38","38","39","39","43"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","","33","","34"]
["Sound pressure level","Cooling","","Low","dBA","35","25","25","26","26","37"]
["","","","Silent operation","dBA","32","22","22","25","25","33"]
["","Heating","","High","dBA","40","38","38","40","40","43"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","","33","","34"]
["Sound pressure level","Heating","","Low","dBA","35","28","28","26","26","37"]
["","","","Silent operation","dBA","32","25","25","23","23","33"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","","6.35","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","","9.5","9.5","9.5","9.5"]
["","التصريف","","","","","18","18","18","18"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","APGS02","ARC470A1","ARC470A1","ARC470A1","ARC470A1","APGS02"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1","V1","V1","V1","V1"]
["","الطور","","","","1~","1~","1~","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - تم اختبار كل الوحدات والتأكد من موافقتها للمقياس ISO5151 (وحدة بلا مجاري هوائية) أو ISO13253 (وحدة بمجاري هوائية)","","","","","(1) - تم اختبار كل الوحدات والتأكد من موافقتها للمقياس ISO5151 (وحدة بلا مجاري هوائية) أو ISO13253 (وحدة بمجاري هوائية)"]
["","","","","","(2) - إنّ جميع المواصفات عرضةً للتغيير من قبل الشركة المصنعة دون إشعار مسبق.","","","","","(2) - إنّ جميع المواصفات عرضةً للتغيير من قبل الشركة المصنعة دون إشعار مسبق."]
["Standard Accessories","دليل التركيب","","","","","1","1","1","1"]
["","جهاز تحكم عن بعد لاسلكي","","","","","1","","1"]
["","بطاريات جافة قياس AA","","","","","2","","2"]
["","دليل التشغيل","","","","","1","1","1","1"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","","","2","2","2","2"]
["","لوح التثبيت","","","","","1","1","1","1"]
["","حامل جهاز التحكم عن بعد","","","","","1","1","1","1"]
["Notes","","","","","","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء","(1) - يحتوي على غازات الاحتباس الحراري المفلورة","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء"]
["Standard Accessories","البطاريات","","","","","","2","","2"]
["","جهاز تحكم عن بعد بالأشعة تحت الحمراء","","","","","","1","","1"]
["","مرشح تنقية الهواء بالتحفيز الضوئي وأباتيت التيتانيوم","","","","","","2","","2"]