{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-J-S / RXG-J"]
[]
[]
[]
[]
["","","","","FTXG25JV1BS / RXG25J2V1B","FTXG35JV1BS / RXG35J2V1B"]
["Cooling capacity","Min.","","kW","1.3","1.4 (1)"]
["","Max.","","kW","3.0","3.8 (1)"]
["","Nom.","","kW","2.5 (1)","3.5 (1)"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35","6.35"]
["","غاز","القطر الخارجي","mm","9.52","9.52"]
["","Drain","OD","mm","18","18"]
["الفعالية الاسمية","نسبة فعالية استهلاك الطاقة","","","4.46","3.93"]
["","عامل الأداء","","","4.36","4.04"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A"]
["","","تدفئة","","A","A"]
["Heating capacity","Nom.","","kW","3.4 (2)","4.0 (2)"]
["","Min.","","kW","1.3","1.4"]
["","Max.","","kW","4.5","5.0"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(2) - التسخين: درجة الحرارة الداخلية 21‏° مئوية للحوجلة الجافة‏؛ درجة الحرارة الخارجية 7‏° مئوية للحوجلة الجافة، 6‏° مئوية للحوجلة الرطبة؛ طول الأنبوب: 5 م","(2) - التسخين: درجة الحرارة الداخلية 21‏° مئوية للحوجلة الجافة‏؛ درجة الحرارة الخارجية 7‏° مئوية للحوجلة الجافة، 6‏° مئوية للحوجلة الرطبة؛ طول الأنبوب: 5 م"]
["","","","","(3) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(3) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]