{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":10,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-JA / RXLG-K"]
[]
[]
[]
[]
["","","","","FTXG25JV1BA / RXLG25K2V1B","FTXG25JV1BA / RXLG25K3V1B","FTXG35JV1BA / RXLG35K2V1B","FTXG35JV1BA / RXLG35K3V1B","FTXG50JV1BA / RXLG50K2V1B","FTXG50JV1BA / RXLG50K3V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.4","1.4","1.7","1.7"]
["","Max.","","kW","3.0","3.0","3.8","3.8","5.3","5.3"]
["","Nom.","","kW","2.5 (3)","2.5 (2)","3.5 (3)","3.5 (2)","5.0 (2)","5.0 (2)"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","غاز","القطر الخارجي","mm","9.52","9.52","9.52","9.52","12.7","12.7"]
["","Drain","OD","mm","16 أو 18","16 أو 18","16 أو 18","16 أو 18","18.0","18.0"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","280","280","445","445","780","780"]
["","نسبة فعالية استهلاك الطاقة","","","4.46","4.46 (1)","3.93","3.93 (1)","3.21 (1)","3.21 (1)"]
["","عامل الأداء","","","4.36","4.36 (1)","4.04","4.04 (1)","3.63 (1)","3.63 (1)"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","A","A","A","A"]
["","","تدفئة","","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","3.4 (4)","3.4 (3)","4.0 (4)","4.0 (3)","5.8 (3)","5.8 (3)"]
["","Min.","","kW","1.3","1.3","1.4","1.4","1.7","1.7"]
["","Max.","","kW","4.5","4.5","5.0","5.0","6.5","6.5"]
["Notes","","","","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - 220 فولت","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - 220 فولت","(4) - 220 فولت","(4) - 220 فولت"]
["","","","","(5) - SL: The silent fan level of the air flow rate setting","(5) - 230 فولت","(5) - SL: The silent fan level of the air flow rate setting","(5) - 230 فولت","(5) - 230 فولت","(5) - 230 فولت"]
["","","","","(6) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","(6) - 240 فولت","(6) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","(6) - 240 فولت","(6) - 240 فولت","(6) - 240 فولت"]
["","","","","(7) - 220 فولت","(7) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(7) - 220 فولت","(7) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(7) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(7) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]
["","","","","(8) - 230 فولت","","(8) - 230 فولت"]
["","","","","(9) - 240 فولت","","(9) - 240 فولت"]
["","","","","(10) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","","(10) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]