{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":7,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-JB"]
[]
[]
[]
[]
["","","","","FTXG25JV1BB","FTXG35JV1BB","FTXG50JV1BB"]
["Sound pressure level","Heating","High","dBA","39","42","44"]
["","","Silent operation","dBA","25","26","32"]
["","","Low","dBA","28","29","35"]
["","Cooling","Silent operation","dBA","22","23","32"]
["","","Low","dBA","25","26","35"]
["","","High","dBA","38","42","44"]
["","","Nom.","dBA","34","36","40"]
["","Cooling","Nom.","dBA","32","34","40"]
["Standard Accessories","مرشح تنقية الهواء بالتحفيز الضوئي وأباتيت التيتانيوم","","","2","2","2"]
["","دليل التشغيل","","","1","1","1"]
["","دليل التركيب","","","1","1","1"]
["","جهاز تحكم عن بعد لاسلكي","","","1","1","1"]
["","البطاريات","","","2","2","2"]
["","حامل جهاز التحكم عن بعد","","","1","1","1"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","2","2","2"]
["","لوح التثبيت","","","1","1","1"]
["","نموذج الورق","","","2","2","2"]
["Piping connections","Liquid","القطر الخارجي","mm","6.35","6.35","6.35"]
["","غاز","القطر الخارجي","mm","9.52","9.52","12.7"]
["","Drain","","","16 أو 18","16 أو 18","18"]
["Power input","Cooling","Nom.","kW","0.018 (3), 0.018 (4), 0.018 (5)","0.026 (3), 0.026 (4), 0.026 (5)","0.032 (3), 0.032 (4), 0.032 (5)"]
["","Heating","Nom.","kW","0.024 (3), 0.024 (4), 0.024 (5)","0.032 (3), 0.032 (4), 0.032 (5)","0.038 (3), 0.038 (4), 0.038 (5)"]
["Sound power level","التبريد","","dBA","56","60","60"]
["","التدفئة","","dBA","57","60","60"]
["Dimensions","Unit","العرض","mm","915","915","915"]
["","","العمق","mm","155","155","155"]
["","","الارتفاع","mm","295","295","295"]
["الغلاف","اللون","","","أسود غير لامع","أسود غير لامع","أسود غير لامع"]
["الوزن","الوحدة","","kg","11","11","11"]
["Power supply","الطور","","","1~","1~","1~"]
["","Frequency","","Hz","50","50","50"]
["","الاسم","","","V1","V1","V1"]
["","Voltage","","V","220-240","220-240","220-240"]
["Notes","","","","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء"]
["","","","","(2) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها.","(2) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها.","(2) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها."]
["","","","","(3) - 220 فولت","(3) - 220 فولت","(3) - 220 فولت"]
["","","","","(4) - 230 فولت","(4) - 230 فولت","(4) - 230 فولت"]
["","","","","(5) - 240 فولت","(5) - 240 فولت","(5) - 240 فولت"]