{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":8,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-JB"]
[]
[]
[]
[]
["","","","","","FTXG25JV1BB","FTXG35JV1BB","FTXG50JV1BB"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","6.8","7.3","8.5"]
["Sound pressure level","Cooling","","Nom.","dBA","32","34","40"]
["Fan","Air flow rate","Heating","Nom.","m³/min","7.9","8.6","9.8"]
["Sound pressure level","Heating","","Nom.","dBA","34","36","40"]
["Power input","Cooling","","Nom.","kW","0.018 (4) (5) (3), 0.018 (4) (5) (3), 0.018 (4) (5) (3)","0.026 (5) (4) (3), 0.026 (5) (4) (3), 0.026 (5) (4) (3)","0.032 (4) (5) (3), 0.032 (4) (5) (3), 0.032 (4) (5) (3)"]
["","Heating","","Nom.","kW","0.024 (4) (3) (5), 0.024 (4) (3) (5), 0.024 (4) (3) (5)","0.032 (4) (3) (5), 0.032 (4) (3) (5), 0.032 (4) (3) (5)","0.038 (3) (5) (4), 0.038 (3) (5) (4), 0.038 (3) (5) (4)"]
["الغلاف","اللون","","","","أسود غير لامع","أسود غير لامع","أسود غير لامع"]
["الأبعاد","الوحدة","","الارتفاع","mm","295","295","295"]
["","","","العرض","mm","915","915","915"]
["","","","العمق","mm","155","155","155"]
["الوزن","الوحدة","","","kg","11","11","11"]
["Fan","Air flow rate","Cooling","High","m³/min","8.8","10.1","10.3"]
["","","","Low","m³/min","4.7","4.6","6.7"]
["","","","Silent operation","m³/min","3.8","3.9","5.7"]
["","","Heating","High","m³/min","9.6","10.8","11.4"]
["","","","Low","m³/min","6.2","6.4","8.1"]
["","","","Silent operation","m³/min","5.4","5.6","7.1"]
["مستوى طاقة الصوت","التبريد","","","dBA","56","60","60"]
["","التدفئة","","","dBA","57","60","60"]
["Sound pressure level","Cooling","","High","dBA","38","42","44"]
["","","","Low","dBA","25","26","35"]
["","","","Silent operation","dBA","22","23","32"]
["","Heating","","High","dBA","39","42","44"]
["","","","Low","dBA","28","29","35"]
["","","","Silent operation","dBA","25","26","32"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.52","9.52","12.7"]
["","التصريف","","","","16 أو 18","16 أو 18","18"]
["Standard Accessories","دليل التركيب","","","","1","1","1"]
["","جهاز تحكم عن بعد لاسلكي","","","","1","1","1"]
["","نموذج الورق","","","","2","2","2"]
["","دليل التشغيل","","","","1","1","1"]
["","البطاريات","","","","2","2","2"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","","2","2","2"]
["","لوح التثبيت","","","","1","1","1"]
["","حامل جهاز التحكم عن بعد","","","","1","1","1"]
["","مرشح تنقية الهواء بالتحفيز الضوئي وأباتيت التيتانيوم","","","","2","2","2"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1","V1"]
["","الطور","","","","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء","(1) - المستوى الصامت: مستوى المروحة الصامت لإعداد معدل تدفق الهواء"]
["","","","","","(2) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها.","(2) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها.","(2) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها."]
["","","","","","(3) - 220 فولت","(3) - 220 فولت","(3) - 220 فولت"]
["","","","","","(4) - 230 فولت","(4) - 230 فولت","(4) - 230 فولت"]
["","","","","","(5) - 240 فولت","(5) - 240 فولت","(5) - 240 فولت"]