{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":7,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXL-JV"]
[]
[]
[]
[]
["","","","","","FTXL25J2V1B","FTXL35J2V1B"]
["Power input","Cooling","","Nom.","kW","0.040 (1) (2) (3), 0.040 (1) (2) (3), 0.040 (1) (2) (3)","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)"]
["","Heating","","Nom.","kW","0.040 (1) (2) (3), 0.040 (1) (2) (3), 0.040 (1) (2) (3)","0.040 (3) (2) (1), 0.040 (3) (2) (1), 0.040 (3) (2) (1)"]
["الغلاف","اللون","","","","أبيض","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","283","283"]
["","","","العرض","mm","770","770"]
["","","","العمق","mm","198","198"]
["الوزن","الوحدة","","","kg","8.00","8.00"]
["Fan","Air flow rate","Cooling","High","m³/min","9.3","9.3"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","7.7","7.7"]
["Fan","Air flow rate","Cooling","Low","m³/min","6.1","6.1"]
["","","","Silent operation","m³/min","4.9","4.9"]
["","","Heating","High","m³/min","10.1","10.1"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","8.4","8.4"]
["Fan","Air flow rate","Heating","Low","m³/min","6.7","6.7"]
["","","","Silent operation","m³/min","5.7","5.7"]
["مستوى طاقة الصوت","التبريد","","","dBA","57","57"]
["","التدفئة","","","dBA","57","57"]
["Sound pressure level","Cooling","","High","dBA","41","41"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","34","34"]
["Sound pressure level","Cooling","","Low","dBA","27","27"]
["","","","Silent operation","dBA","23","23"]
["","Heating","","High","dBA","41","41"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","35","35"]
["Sound pressure level","Heating","","Low","dBA","29","29"]
["","","","Silent operation","dBA","26","26"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.50","9.50"]
["","التصريف","","","","18","18"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","ARC433A87, ARC466A9","ARC433A87, ARC466A9"]
["Standard Accessories","دليل التركيب","","","","1","1"]
["","جهاز تحكم عن بعد لاسلكي","","","","1","1"]
["","دليل التشغيل","","","","1","1"]
["","مرشح أباتيت التيتانيوم المزيل للروائح","","","","2","2"]
["","البطاريات","","","","2","2"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","","2","2"]
["","لوح التثبيت","","","","1","1"]
["","حامل جهاز التحكم عن بعد","","","","1","1"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1"]
["","الطور","","","","1~","1~"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - 220 فولت","(1) - 220 فولت"]
["","","","","","(2) - 230 فولت","(2) - 230 فولت"]
["","","","","","(3) - 240 فولت","(3) - 240 فولت"]
["","","","","","(4) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها.","(4) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها."]