{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":11,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N / 5MXM-A8"]
[]
[]
[]
[]
["","","","","FTXM20N2V1B / FTXM71N2V1B / 5MXM90A2V1B8","FTXM20N2V1B / FTXM20N2V1B / FTXM25N2V1B / FTXM25N2V1B / 5MXM90A2V1B8","FTXM20N2V1B / FTXM20N2V1B / FTXM50N2V1B / 5MXM90A2V1B8","FTXM20N2V1B / FTXM25N2V1B / FTXM42N2V1B / 5MXM90A2V1B8","FTXM20N2V1B / FTXM35N2V1B / FTXM35N2V1B / 5MXM90A2V1B8","FTXM25N2V1B / FTXM25N2V1B / FTXM42N2V1B / 5MXM90A2V1B8","FTXM42N2V1B / FTXM50N2V1B / 5MXM90A2V1B8"]
["Cooling capacity","Nom.","","kW","8.00","7.80","8.00","8.00","8.00","8.00","8.00"]
["Heating capacity","Nom.","","kW","10.00","10.00","10.00","10.00","10.00","10.00","10.00"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","3.33","4.15","3.82","3.71","3.73","3.72","3.34"]
["","عامل الأداء","","","3.69","4.58","4.28","4.08","3.99","4.09","3.74"]
["","استهلاك الطاقة السنوي","","kWh","1202","940","1047","1077","1073","1075","1199"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","A","A","A","A","A"]
["","","تدفئة","","A","A","A","A","A","A","A"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A++","A++","A++","A++","A++","A++","A++"]
["","الاستطاعة","Pdesign","kW","8.00","7.80","8.00","8.00","8.00","8.00","8.00"]
["","SEER","","","6.84","7.55","7.29","7.17","7.18","7.18","6.85"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","410","366","387","391","392","391","411"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A+","A+","A+","A+","A+","A+","A+"]
["","الاستطاعة","Pdesign","kW","4.50","6.46","6.46","5.60","6.46","5.60","5.20"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","4.26","4.50","4.34","4.35","4.20","4.36","4.21"]
["","Pdh استطاعة التدفئة عند -10°","","kW","3.84","5.02","4.98","4.47","4.97","4.48","4.19"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","1478","2010","2083","1803","2152","1799","1731"]