{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":11,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / RZAG-A"]
[]
[]
[]
[]
["","","","","FTXM35R2V1B / RZAG35A2V1B","FTXM50R2V1B / RZAG35A2V1B","FTXM35R5V1B / RZAG35A2V1B","FTXM50R2V1B / RZAG50A2V1B","FTXM60R2V1B / RZAG50A2V1B","FTXM71R2V1B / RZAG60A2V1B","FTXM60R2V1B / RZAG60A2V1B"]
["Cooling capacity","Min.","","kW","1.6","1.60","1.6","1.7","1.70","1.70","1.7"]
["","Max.","","kW","5.0","5.00","5.0","6.0","6.00","6.80","6.8"]
["","Nom.","","kW","3.5","3.50","3.5","5.0","5.00","6.00","6.0"]
["تبريد المساحة","SEER","","","7.70","7.76","7.70","7.41","7.53","6.90","6.90"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","159","158","159","236","232","304","304"]
["","الاستطاعة","Pdesign","kW","3.50","3.50","3.50","5.00","5.00","6.00","6.00"]
["","فئة فعالية استهلاك الطاقة","","","A++","A++","A++","A++","A++","A++","A++"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","2.60","2.60","2.60","4.50","4.50","4.50","4.60"]
["","SCOP/A","","","4.60","4.68","4.60","4.60","4.69","4.40","4.35"]
["","فئة فعالية استهلاك الطاقة","","","A++","A++","A++","A++","A++","A+","A+"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","790","778","790","1,369","1,344","1,433","1,480"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","407","405","407","625","619","857","857"]
["","نسبة فعالية استهلاك الطاقة","","","4.30","4.32","4.30","4.00","4.04","3.50","3.50"]
["","عامل الأداء","","","3.85","3.93","3.85","4.00","4.08","3.68","3.61"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","A","A","A","A","A"]
["","","تدفئة","","A","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","4.00","4.00","4.00","6.00","6.00","7.00","7.00"]
["","Min.","","kW","1.40","1.40","1.40","1.50","1.50","1.60","1.60"]
["","Max.","","kW","5.30","5.30","5.30","6.50","6.50","7.50","7.50"]