{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":14,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-L / RXP-L"]
[]
[]
[]
[]
["","","","","FTXP20L2V1B / RXP20L5V1B","FTXP20L5V1B / RXP20L5V1B","FTXP20L2V1B / RXP20L2V1B","FTXP25L2V1B / RXP25L5V1B","FTXP25L5V1B / RXP25L5V1B","FTXP25L2V1B / RXP25L2V1B","FTXP35L2V1B / RXP35L5V1B","FTXP35L5V1B / RXP35L5V1B","FTXP50L2V1B / RXP50L2V1B","FTXP71L2V1B / RXP71L2V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","","1.3","1.3","","1.3","1.3","","2.3"]
["","Max.","","kW","2.6","2.6","","3.0","3.0","","4.0","4.0","","7.3"]
["","Nom.","","kW","2.00","2.00","","2.50","2.50","","3.50","3.50","","7.1"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","","","","","","","","","","1,345"]
["","نسبة فعالية استهلاك الطاقة","","","4.02","4.02","","3.83","3.83","","3.49","3.49","","2.64"]
["","عامل الأداء","","","4.77","4.77","","4.36","4.36","","4.02","4.02","","3.19"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","","A","A","","A","A"]
["","","تدفئة","","A","A","","A","A","","A","A"]
["Heating capacity","Nom.","","kW","2.50","2.50","","3.00","3.00","","4.00","4.00","","8.2"]
["","Min.","","kW","1.30","1.30","","1.30","1.30","","1.30","1.30","","2.3"]
["","Max.","","kW","3.50","3.50","","4.00","4.00","","4.80","4.80","","9.00"]
["Notes","","","","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0","","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0","","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0","","(1) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data"]
["Outdoor unit","","","","","","RXP20L2V1B","","","RXP25L2V1B"]
["Cooling capacity","Min.","","kW","","","1.3","","","1.3","","","1.7"]
["","Nom.","","kW","","","2.00","","","2.50","","","5.0"]
["","Max.","","kW","","","2.6","","","3.0","","","6.0"]
["Heating capacity","Min.","","kW","","","1.30","","","1.30","","","1.7"]
["","Nom.","","kW","","","2.50","","","3.00","","","6.0"]
["","Max.","","kW","","","3.50","","","4.00","","","7.70"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","","","4.02","","","3.83","","","3.61"]
["","عامل الأداء","","","","","4.77","","","4.36","","","3.80"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","","","A","","","A"]
["","","تدفئة","","","","A","","","A"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","","","A++","","","A++","","","A++"]
["","الاستطاعة","Pdesign","kW","","","2.00","","","2.50","","","5.00"]
["","SEER","","","","","6.79","","","6.92","","","6.72"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","","104","","","127","","","261"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","","","A++","","","A++","","","A+"]
["","الاستطاعة","Pdesign","kW","","","2.20","","","2.40","","","4.60"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","","","4.65","","","4.61","","","4.10"]
["","Pdh استطاعة التدفئة عند -10°","","kW","","","1.99","","","2.10","","","4.12"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","","662","","","728","","","1570"]
["نطاق كفاءة استخدام الطاقة","","","","","","A+++ ~ D","","","A+++ ~ D","","","A+++ ~ D"]
["الفعالية الإسمية","استهلاك الطاقة السنوي","","kWh","","","","","","","","","693"]