{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Sound pressure level","Heating","","High","dBA","43"]
["","","","متوسط","dBA","35"]
["","","","Silent operation","dBA","21"]
["","","","Low","dBA","26"]
["","Cooling","","متوسط","dBA","35"]
["","","","Silent operation","dBA","21"]
["","","","Low","dBA","26"]
["","","","High","dBA","43"]
["Standard Accessories","دليل التركيب","","","","1"]
["","دليل التشغيل","","","","1"]
["","جهاز تحكم عن بعد لاسلكي","","","","1"]
["","بطاريات جافة قياس AAA","","","","2"]
["","حامل جهاز التحكم عن بعد","","","","1"]
["","لوح التثبيت","","","","1"]
["","مرشح أباتيت التيتانيوم المزيل للروائح","","","","2"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","","2"]
["أنظمة التحكم","Wired remote control","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Piping connections","Liquid","","القطر الخارجي","mm","6.35"]
["","غاز","","القطر الخارجي","mm","9.50"]
["","Drain","","","","16 (القطر الداخلي لخرطوم التوصيل)"]
["Power input","Cooling","","Nom.","kW","0.030"]
["","Heating","","Nom.","kW","0.035"]
["Sound power level","التبريد","","","dBA","58"]
["","التدفئة","","","dBA","58"]
["Dimensions","Unit","","العرض","mm","770"]
["","","","العمق","mm","225"]
["","","","الارتفاع","mm","285"]
["الغلاف","اللون","","","","White"]
["الوزن","الوحدة","","","kg","9.0"]
["Power supply","الطور","","","","1~"]
["","Frequency","","","Hz","50"]
["","الاسم","","","","V1"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]
["Power input","Cooling","","Nom.","kW","","0.03"]
["","Heating","","Nom.","kW","","0.035"]
["الغلاف","اللون","","","","","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","","285"]
["","","","العرض","mm","","770"]
["","","","العمق","mm","","225"]
["الوزن","الوحدة","","","kg","","9"]
["Fan","Air flow rate","Cooling","High","m³/min","","11.4"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","","8.2"]
["Fan","Air flow rate","Cooling","Low","m³/min","","5.4"]
["","","","Silent operation","m³/min","","4.3"]
["","","Heating","High","m³/min","","10.8"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","","7.8"]
["Fan","Air flow rate","Heating","Low","m³/min","","5.8"]
["","","","Silent operation","m³/min","","4.9"]
["مستوى طاقة الصوت","التبريد","","","dBA","","58"]
["","التدفئة","","","dBA","","58"]
["Sound pressure level","Cooling","","High","dBA","","43"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","","35"]
["Sound pressure level","Cooling","","Low","dBA","","26"]
["","","","Silent operation","dBA","","21"]
["","Heating","","High","dBA","","43"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","","35"]
["Sound pressure level","Heating","","Low","dBA","","26"]
["","","","Silent operation","dBA","","21"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","","6.35"]
["","غاز","","القطر الخارجي","mm","","9.5"]
["","التصريف","","","","","16 (القطر الداخلي لخرطوم التوصيل)"]
["أنظمة التحكم","Infrared remote control","","","","","ARC480A11"]
["أنظمة التحكم","جهاز تحكم عن بُعد سلكي","","","","","BRC944B2, BRC073A1"]
["Standard Accessories","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["وحدة التزويد بالطاقة","الاسم","","","","","V1"]
["","الطور","","","","","1~"]
["Power supply","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]