{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Power input","Cooling","","Nom.","kW","0.03","0.03"]
["","Heating","","Nom.","kW","0.035","0.035"]
["الغلاف","اللون","","","","أبيض","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","285","285"]
["","","","العرض","mm","770","770"]
["","","","العمق","mm","225","225"]
["الوزن","الوحدة","","","kg","9","9"]
["Fan","Air flow rate","Cooling","High","m³/min","10.6","11.4"]
["مروحة","معدل تدفق الهواء","تبريد","متوسط","m³/min","7.7","8.2"]
["Fan","Air flow rate","Cooling","Low","m³/min","5.3","5.4"]
["","","","Silent operation","m³/min","4.3","4.3"]
["","","Heating","High","m³/min","11.2","10.8"]
["مروحة","معدل تدفق الهواء","تدفئة","متوسط","m³/min","8","7.8"]
["Fan","Air flow rate","Heating","Low","m³/min","5.8","5.8"]
["","","","Silent operation","m³/min","4.9","4.9"]
["مستوى طاقة الصوت","التبريد","","","dBA","58","58"]
["","التدفئة","","","dBA","58","58"]
["Sound pressure level","Cooling","","High","dBA","43","43"]
["مستوى ضغط الصوت","تبريد","","متوسط","dBA","35","35"]
["Sound pressure level","Cooling","","Low","dBA","26","26"]
["","","","Silent operation","dBA","21","21"]
["","Heating","","High","dBA","43","43"]
["مستوى ضغط الصوت","تدفئة","","متوسط","dBA","35","35"]
["Sound pressure level","Heating","","Low","dBA","26","26"]
["","","","Silent operation","dBA","21","21"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.5","9.5"]
["","التصريف","","","","16 (القطر الداخلي لخرطوم التوصيل)","16 (القطر الداخلي لخرطوم التوصيل)"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","ARC480A11","ARC480A11"]
["","جهاز تحكم عن بُعد سلكي","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standard Accessories","دليل التركيب","","","","1","1"]
["","جهاز تحكم عن بعد لاسلكي","","","","1","1"]
["","بطاريات جافة قياس AAA","","","","2","2"]
["","دليل التشغيل","","","","1","1"]
["","مرشح أباتيت التيتانيوم المزيل للروائح","","","","2","2"]
["","مسامير لولبية لتثبيت الوحدة الداخلية","","","","2","2"]
["","لوح التثبيت","","","","1","1"]
["","حامل جهاز التحكم عن بعد","","","","1","1"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1"]
["","الطور","","","","1~","1~"]
["Power supply","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية","(1) - انظر المخطط المنفصل الخاص بالبيانات الكهربائية"]