{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-M / RXTP-A"]
[]
[]
[]
[]
["","","","","FTXTP25M5V1B / RXTP25A2V1B","FTXTP35M5V1B / RXTP35A2V1B"]
["Cooling capacity","Min.","","kW","0.80","0.80"]
["","Nom.","","kW","2.50","3.50"]
["","Max.","","kW","4.00","4.40"]
["Heating capacity","Min.","","kW","1.20","1.20"]
["","Nom.","","kW","3.20","4.00"]
["","Max.","","kW","6.20","6.70"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","4.40","3.80"]
["","عامل الأداء","","","4.95","4.44"]
["","استهلاك الطاقة السنوي","","kWh","284","461"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","A","A"]
["","","تدفئة","","A","A"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","A++","A++"]
["","الاستطاعة","Pdesign","kW","2.50","3.50"]
["","SEER","","","7.10","7.20"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","123","170"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","A++","A++"]
["","الاستطاعة","Pdesign","kW","2.50","3.00"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","4.93","4.81"]
["","Pdh استطاعة التدفئة عند -10°","","kW","2.50","3.00"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","710","873"]