{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-F / RXM-N"]
[]
[]
[]
[]
["","","","","FVXM50FV1B9 / RXM50N2V1B","FVXM50FV1B / RXM50N2V1B"]
["Cooling capacity","Min.","","kW","1.40"]
["","Max.","","kW","5.60"]
["","Nom.","","kW","5.00"]
["تبريد المساحة","SEER","","","6.80"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","257"]
["","الاستطاعة","Pdesign","kW","5.00"]
["","فئة فعالية استهلاك الطاقة","","","A++"]
["تدفئة المساحة (مناخ معتدل)","الاستطاعة","Pdesign","kW","4.20"]
["","SCOP/A","","","4.00"]
["","فئة فعالية استهلاك الطاقة","","","A+"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","1,471"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","773"]
["","نسبة فعالية استهلاك الطاقة","","","3.23"]
["","عامل الأداء","","","3.63"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A"]
["","","تدفئة","","A"]
["Heating capacity","Nom.","","kW","5.80"]
["","Min.","","kW","1.40"]
["Notes","","","","(1) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","(2) - See separate drawing for electrical data"]
["","","","","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0"]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Outdoor unit","","","","","RXM50N2V1B"]
["Cooling capacity","Min.","","kW","","1.40"]
["","Nom.","","kW","","5.00"]
["","Max.","","kW","","5.60"]
["Heating capacity","Min.","","kW","","1.40"]
["","Nom.","","kW","","5.80"]
["الفعالية الإسمية","نسبة فعالية استهلاك الطاقة","","","","3.23"]
["","عامل الأداء","","","","3.63"]
["","استهلاك الطاقة السنوي","","kWh","","773"]
["الفعالية الاسمية","التوجيه الخاص بملصق الطاقة","تبريد","","","A"]
["","","تدفئة","","","A"]
["تبريد المساحة","فئة فعالية استهلاك الطاقة","","","","A++"]
["","الاستطاعة","Pdesign","kW","","5.00"]
["","SEER","","","","6.80"]
["تدفئة المساحة","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","257"]
["تدفئة المساحة (مناخ معتدل)","فئة فعالية استهلاك الطاقة","","","","A+"]
["","الاستطاعة","Pdesign","kW","","4.20"]
["","تدفئة المساحة (مناخ معتدل)-=-SCOP/A","","","","4.00"]
["","Pdh استطاعة التدفئة عند -10°","","kW","","3.81"]
["","استهلاك الطاقة السنوي","","كيلو واط ساعي/سنة","","1471"]
["نطاق كفاءة استخدام الطاقة","","","","","A+++ ~ D"]