{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":12,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-F / RXM-N9"]
[]
[]
[]
[]
["","","","","FVXM25FV1B / RXM25N2V1B9","FVXM25FV1B / RXM25N5V1B9","FVXM25FV1B9 / RXM25N2V1B9","FVXM35FV1B / RXM35N2V1B9","FVXM35FV1B / RXM35N5V1B9","FVXM35FV1B9 / RXM35N2V1B9","FVXM50FV1B / RXM50N2V1B9","FVXM50FV1B9 / RXM50N2V1B9"]
["Cooling capacity","Min.","","kW","1.30","1.30","1.30","1.40","1.40","1.40","1.40","1.40"]
["","Max.","","kW","3.00","3.00","3.00","3.80","3.80","3.80","5.60","5.60"]
["","Nom.","","kW","2.50","2.50","2.50","3.50","3.50","3.50","5.00","5.00"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","298","298","298","545","545","545","773","773"]
["","نسبة فعالية استهلاك الطاقة","","","4.20","4.20","4.20","3.21","3.21","3.21","3.23","3.23"]
["","عامل الأداء","","","4.42","4.42","4.42","3.78","3.78","3.78","3.63","3.63"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A","A","A","A","A","A","A"]
["","","تدفئة","","A","A","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","3.40","3.40","3.40","4.50","4.50","4.50","5.80","5.80"]
["","Min.","","kW","1.30","1.30","1.30","1.40","1.40","1.40","1.40","1.40"]
["","Max.","","kW","4.50","4.50","4.50","5.00","5.00","5.00","8.10","8.10"]
["Notes","","","","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data"]
["","","","","(2) - انظر الرسم المنفصل لنطاق التشغيل","(2) - انظر الرسم المنفصل لنطاق التشغيل","(2) - انظر الرسم المنفصل لنطاق التشغيل","(2) - انظر الرسم المنفصل لنطاق التشغيل","(2) - انظر الرسم المنفصل لنطاق التشغيل","(2) - انظر الرسم المنفصل لنطاق التشغيل","(2) - انظر الرسم المنفصل لنطاق التشغيل","(2) - انظر الرسم المنفصل لنطاق التشغيل"]
["","","","","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB، درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0م.","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0","(3) - استطاعات التبريد الإسمية تستند إلى: درجة الحرارة الداخلية: 27‏° مئوية CDB، و19‏° مئوية CWB؛ درجة الحرارة الخارجية: 35‏° مئوية CDB؛ طول أنبوب سائل التبريد المكافئ: 5م، فرق المستوى: 0"]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]