{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":10,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXS-F / RXL-J"]
[]
[]
[]
[]
["","","","","FVXS25FV1B / RXL25J3V1B (Preliminary)","FVXS25FV1B / RXL25J2V1B","FVXS35FV1B / RXL35J2V1B","FVXS35FV1B / RXL35J3V1B","FVXS50FV1B / RXL50J2V1B","FVXS50FV1B / RXL50J3V1B"]
["Cooling capacity","Min.","","kW","","1.3","1.4","1.4","1.4","1.4"]
["","Max.","","kW","","3.0","3.8","3.8","5.6","5.6"]
["","Nom.","","kW","","2.5 (3)","3.5 (3)","3.5 (2)","5.0 (2)","5.0 (2)"]
["Piping connections","Liquid","القطر الخارجي","mm","","6.35","6.35","6.35","6.35","6.35"]
["","غاز","القطر الخارجي","mm","","9.5","9.5","9.5","12.7","12.7"]
["","Drain","OD","mm","","","","20.0","20.0","20.0"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","","285","407","510","775","775"]
["Heating capacity","Nom.","","kW","","3.4 (4)","4.5 (4)","4.5 (3)","5.8 (3)","5.8 (3)"]
["","Min.","","kW","","1.3","1.4","1.4","1.4","1.4"]
["","Max.","","kW","","4.5","5.0","5.0","8.1","8.1"]
["Notes","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["الفعالية الاسمية","نسبة فعالية استهلاك الطاقة","","","","4.39","4.30","3.43 (1)","3.23 (1)","3.23 (1)"]
["","عامل الأداء","","","","3.43","3.69","3.69 (1)","3.63 (1)","3.63 (1)"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","A","A","A","A","A"]
["","","تدفئة","","","B","A","A","A","A"]
["Notes","","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m (horizontal)","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m (horizontal)","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(4) - 220 فولت","(4) - 220 فولت","(4) - 220 فولت"]
["","","","","","(5) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(5) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(5) - 230 فولت","(5) - 230 فولت","(5) - 230 فولت"]
["","","","","","","","(6) - 240 فولت","(6) - 240 فولت","(6) - 240 فولت"]
["","","","","","","","(7) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(7) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(7) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]