{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXS-F / RXL-M3"]
[]
[]
[]
[]
["","","","","FVXS25FV1B / RXL25M3V1B","FVXS35FV1B / RXL35M3V1B"]
["Cooling capacity","Nom.","","kW","2.5","3.5"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","370","535"]
["","نسبة فعالية استهلاك الطاقة","","","3.38","3.27"]
["","عامل الأداء","","","3.78","3.46"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","A","A"]
["","","تدفئة","","A","B"]
["Heating capacity","Nom.","","kW","4.5","5.6"]
["Notes","","","","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط","(1) - نسبة فعالية استهلاك الطاقة/عامل الأداء بحسب Eurovent 2012، للاستخدام خارج دول الاتحاد الأوروبي فقط"]
["","","","","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(2) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]
["","","","","(3) - 220 فولت","(3) - 220 فولت"]
["","","","","(4) - 230 فولت","(4) - 230 فولت"]
["","","","","(5) - 240 فولت","(5) - 240 فولت"]
["","","","","(6) - للحصول على الحد الأدنى المقدّر من استطاعة التدفئة يتم ضبط مروحة الوحدة الداخلية إلى العتبة SL","(6) - للحصول على الحد الأدنى المقدّر من استطاعة التدفئة يتم ضبط مروحة الوحدة الداخلية إلى العتبة SL"]
["","","","","(7) - استطاعة التدفئة الأعظمية عند درجة حرارة خارجية -15° مئوية","(7) - استطاعة التدفئة الأعظمية عند درجة حرارة خارجية -15° مئوية"]