{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXS-F / RXS-J"]
[]
[]
[]
[]
["","","","","FVXS25FV1B / RXS25J2V1B (Preliminary)","FVXS35FV1B / RXS35J2V1B","FVXS50FV1B / RXS50J2V1B"]
["Cooling capacity","Min.","","kW","","1.4","1.4"]
["","Max.","","kW","","3.8","5.6"]
["","Nom.","","kW","","3.44 (3)","5.0 (3)"]
["Piping connections","Liquid","القطر الخارجي","mm","","6.35","6.35"]
["","غاز","القطر الخارجي","mm","","9.5","12.7"]
["","Drain","OD","mm","","20.0","20.0"]
["الفعالية الاسمية","استهلاك الطاقة السنوي","","kWh","","510","775"]
["Heating capacity","Nom.","","kW","","4.42 (4)","5.8 (4)"]
["","Min.","","kW","","1.4","1.4"]
["","Max.","","kW","","5.0","8.1"]
["Notes","","","","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)","(1) - ملصق الطاقة: مدرج من A (أعلى فعالية) إلى G (أقل فعالية)"]
["","","","","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)","(2) - استهلاك الطاقة السنوي: استناداً إلى معدل استخدام 500 ساعة تشغيل في السنة بالحمل الكامل (الشروط الأسمية)"]
["","","","","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(3) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(5) - كافة البيانات المذكورة معلومات أولية","(5) - 220 فولت","(5) - 220 فولت"]
["الفعالية الاسمية","نسبة فعالية استهلاك الطاقة","","","","3.43","3.23"]
["","عامل الأداء","","","","3.69","3.63"]
["","التوجيه الخاص بملصق الطاقة","تبريد","","","A","A"]
["","","تدفئة","","","A","A"]
["Notes","","","","","(6) - 230 فولت","(6) - 230 فولت"]
["","","","","","(7) - 240 فولت","(7) - 240 فولت"]
["","","","","","(8) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي","(8) - الفعالية الإسمية: التبريد عند 35°/27° حمل إسمي، التدفئة عند 7°/20° حمل إسمي"]