{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":8,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXS-F"]
[]
[]
[]
[]
["","","","","","FVXS25FV1B","FVXS35FV1B","FVXS50FV1B"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","8.2","8.5","10.7"]
["Sound pressure level","Cooling","","Nom.","dBA","32","33","40"]
["Fan","Air flow rate","Heating","Nom.","m³/min","6.9","7.3","10.1"]
["Sound pressure level","Heating","","Nom.","dBA","32","33","40"]
["الغلاف","اللون","","","","أبيض","أبيض","أبيض"]
["الأبعاد","الوحدة","","الارتفاع","mm","600","600","600"]
["","","","العرض","mm","700","700","700"]
["","","","العمق","mm","210","210","210"]
["الوزن","الوحدة","","","kg","14","14","14"]
["Fan","Air flow rate","Cooling","High","m³/min","8.2","8.5","10.7"]
["","","","Low","m³/min","4.8","4.9","7.8"]
["","","","Silent operation","m³/min","4.1","4.5","6.6"]
["","","Heating","High","m³/min","8.8","9.4","11.8"]
["","","","Low","m³/min","5","5.2","8.5"]
["","","","Silent operation","m³/min","4.4","4.7","7.1"]
["مستوى طاقة الصوت","التبريد","","","dBA","52","52","60"]
["","التدفئة","","","dBA","52","52","60"]
["Sound pressure level","Cooling","","High","dBA","38","39","44"]
["","","","Low","dBA","26","27","36"]
["","","","Silent operation","dBA","23","24","32"]
["","Heating","","High","dBA","38","39","45"]
["","","","Low","dBA","26","27","36"]
["","","","Silent operation","dBA","23","24","32"]
["وصلات الأنابيب","سائل","","القطر الخارجي","mm","6.35","6.35","6.35"]
["","غاز","","القطر الخارجي","mm","9.5","9.52","12.7"]
["","التصريف","","","","20","20","20"]
["أنظمة التحكم","جهاز تحكم عن بُعد بالأشعة تحت الحمراء","","","","ARC452A1","ARC452A1","ARC452A1"]
["Standard Accessories","دليل التركيب","","","","1","1","1"]
["","مرشح تنقية الهواء","","","","2"]
["","جهاز تحكم عن بعد لاسلكي","","","","1","1","1"]
["","دليل التشغيل","","","","1","1","1"]
["","البطاريات","","","","2","2","2"]
["","خرطوم الصرف","","","","1","1","1"]
["","حامل جهاز التحكم عن بعد","","","","1","1","1"]
["","شريط عازل حرارياً","","","","2","2","2"]
["وحدة التزويد بالطاقة","الاسم","","","","V1","V1","V1"]
["","الطور","","","","1~","1~","1~"]
["Power supply","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220 فولت","(1) - 220 فولت"]
["","","","","","(2) - 230 فولت","(2) - 230 فولت"]
["","","","","","(3) - 240 فولت","(3) - 240 فولت"]
["","","","","","(4) - عند التوصيل بوحدة خارجية متعددة الأنظمة، راجع مواصفات الوحدة الخارجية المتعددة المراد توصيلها."]
["Standard Accessories","مرشح ضخ الهواء","","","","","1","1"]